Installing the Reader Harness

| Print out this category

Installation Procedure
Installing the Reader Harness
1) Remove the power cord clamp. (100/120V only)
1 Screw
2) Remove the power cord.
3) Remove the rear cover.
4 Screws
4 Claws
4) Remove the left rear cover.
4 Screws
2 Claws
5) Remove the connector cover.
1 Screw
6) When the cassette pedestal is installed, remove the connector.
7) Remove the lower rear cover.
4 Screws
3 Claws
8) Unlock the wire saddles and stretch the folded harness as shown.
9) Joint 1 connector of the heater harness B to the harness connector of the reader unit.
10) Attach the 4 supplied wire saddles (middle).
11) Attach the heater harness B.
5 Wire saddles (middle)
Caution:
Route the heater harness B as shown in the figure below.
12) Joint the connector to J1105 of the heater PCB.