Selecting the Site of Installation

| Print out this category

﻿Making Pre-Checks
Selecting the Site of Installation
The followings are the condition for installation environment.
It is better to see the planned location of installation before carrying the host machine in the user site.
1) The host machine can singly connect to the outlet of rated +/-10V, 15A or more.
2) The installation site must be in the following environment. Especially, avoid installing the machine near the faucet, water boiler, humidifier, or refrigerator.
Guaranteed range for operation Temperature: 2.5 to 37.5 deg C
Guaranteed range for image Temperature: 15.0 to 30.0 deg C, Humidity: 10 to 80%RH
3) Avoid installing the machine near fire, in an area subject to dust or ammonia gas. When installing the machine in a place exposed to direct rays of the sun, it is recommended that curtains be hung over the windows.
4) The amount of ozone generated during use of the machine is below the harmful level.However, if the machine is used for a long time in a poor-ventilated room, ozone may smell.To keep the work environment comfortable, the room must be well-ventilated properly.
5) None of the machine feet should float. The machine must be held level constantly.
6) Install the machine in a well-ventilated place. Do not install the machine close to the ventilation duct of the room.
7) The machine must be installed at least 10 cm away from the surrounding walls and there must be an adequate space for operating the machine.
When the option is not attached
When the Inner Finisher-D1 and Paper Deck Unit-B2 is attached
When the Inner Finisher-D1, Inner Hole Puncher-A1 and Paper Deck Unit-B2 is attached
When the Booklet Finisher-G1, External 2 Hole Puncher-B2, Buffer Pass Unit-H1 and Paper Deck Unit-B2 is attached