﻿Removing the Cassette Pickup Roller

| Print out this category

Removing the Cassette Pickup Roller
CAUTION:
Do not touch the roller surface during work.
1) Draw out the cassette from the main unit.
2) Open the right cover.
3) Remove the leaf spring with your fingers.
4) Remove the cassette pickup roller.
1 claw
NOTE:
When replacing the consumable parts, be sure to clear the parts counter.
- Cassette 1 (COPIER > COUNTER > DRBL-1 > C1-PU-RL)
- Cassette 2 (COPIER > COUNTER > DRBL-1 > C2-PU-RL)