Outline

| Print out this category

Waste toner container
Outline
Residual toner adhered on the photosensitive drum without being transferred to a paper is scraped off by the cleaning blade in contact with the photosensitive drum, then fed into the waste toner container by the waste toner feed screw.
The waste toer container is supported by a spring. If the waste toner container sinks down lower than specified with the weight of collected toner, the waste toner full sensor (S17) detects the waste toner container full.

S17 | Waste toner full sensor