E-RDS setting items﻿

| Print out this category

E-RDS-related setting items (service mode)
E-RDS setting items﻿

Item | Description
E-RDS ([Lv.1] COPIER > Function > INSTALL) | Set use/ no use of Embedded-RDS function 0: Function not used / 1: Function used e-Maintenance/ imageWARE Remote system to send device information, counter data, error statuses to the UGW. Default : 0 (Function not used)
RGW-ADR ([Lv.1] COPIER > Function > INSTALL) | URL setting of UGW Max 128 characters Default : https://a01.ugwdevice.net/ugw/agentif01
RGW-PORT ([Lv.1] COPIER > Function > INSTALL) | Set port number of UGW Validation : 1 to 65535 Default : 443
COM-TEST ([Lv.1] COPIER > Function > INSTALL) | Execution of a communication test with UGW / Display of the result Perform Communication test with UGW and set "OK!" or "NG!" as the result.

COM-LOG
([Lv.1] COPIER > Function > INSTALL)

Display of detailed information about a communication error with UGW
Error information of a connection failure with UGW is displayed.
Error occurrence date and time, error code, and detailed error information are displayed.
Max 30 latest loggings retained
Max 128 characters for Error information.

ERDS-DAT ([Lv.1] COPIER > Function > CLEAR) | Initialization of E-RDS SRAM data SRAM data of E-RDS is initialized and returned to the factory setting value at shipment.
CA-KEY ([Lv.2] COPIER > Function > CLEAR) | Initialization of CA certificate When the power is turned OFF/ ON after execution, the CA certificate in the factory setting is automatically installed.