NETWORK

| Print out this category

NETWORK

COPIER>OPTION>NETWORK
RAW-DATA | Setting of received data print mode
Lv.2 | Details | To set print mode for the received image data. This item is used to identify the cause whether it's due to image data or image processing in the case of trouble with received image.
Use case | When received image trouble occurs
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to set the value back to "0: Normal print operation" after recovering from the trouble.
Display/adj/set range | 0 to 1 0: Normal print operation, 1: Print with original data without image processing
Default value | 0
IFAX-LIM | No. of max print lines at IFAX reception

Lv.2

Details

To set the maximum number of lines for e-mail text to be printed when receiving IFAX.
Setting of this item can prevent endless printing of the attached file data in the case of receiving an error e-mail or failure in interpretation of the context.
Selecting 0 prints the header/footer in 1 sheet when receiving e-mail text without attached file.

Use case | When preventing endless print in the case of failure in reception
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 999 0: E-mail text not printed, 999: Unlimited
Default value | 500
SMTPTXPN | Setting of SMTP TX port number
Lv.2 | Details | To set SMTP transmission port number.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 65535
Default value | 25
SMTPRXPN | Setting of SMTP reception port number
Lv.2 | Details | To set SMTP reception port number.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 65535
Default value | 25
POP3PN | Setting of POP3 reception port number
Lv.2 | Details | To set POP3 reception port number.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 65535
Default value | 110
FTPTXPN | Specification of SEND port (FTP) number
Lv.2 | Details | To specify address port (FTP) number for SEND.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 65535
Default value | 21
NW-SPEED | Setting of network data transfer speed
Lv.2 | Details | To set the data transfer speed when the service network is connected. When downloading the firmware through network, use 0 in the normal operation. When fixed to 100Base-TX/10Base-T for any reason, change the setting.
Use case | When fixing the communication speed
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: Auto, 1: 100Base-TX, 2: 10Base-T
Default value | 0
STS-PORT | ON/OFF of TOT sync status communication port
Lv.2 | Details | To set ON/OFF for Inquiry/Response (sync)-mode status communication port with T.O.T. Select ""1: ON"" in the case of connecting the PC and the machine with the cross cable while Service NAVI is used.
Use case | When the Service NAVI is used
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
Related service mode | COPIER> OPTION> NETWORK> CMD-PORT
Supplement/memo | T.O.T: TUIF over TCP. Communication protocol to be used for communication with the built-in application (UI) and the internal application such as COPY/ SEND/ BOX, etc. (Canon's own protocol).
CMD-PORT | ON/OFF TOTasync command communication port
Lv.2 | Details | To set ON/OFF for asynchronous command communication port with T.O.T. Select ""1: ON"" in the case of connecting the PC and the machine with the cross cable while Service NAVI is used.
Use case | When the Service NAVI is used
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
Related service mode | COPIER> OPTION> NETWORK> STS-PORT
Supplement/memo | T.O.T: TUIF over TCP. Communication protocol to be used for communication with the built-in application (UI) and the internal application such as COPY/ SEND/ BOX, etc. (Canon's own protocol).
NS-CMD5 | Limit CRAM-MD5 auth method at SMTP auth
Lv.2 | Details | To restrict use of CRAM-MD5 authentication method at the time of SMTP authentication.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: SMTP server-dependent, 1: Not used
Default value | 0
Supplement/memo | SMTP authentication: Protocol in which user authentication function is added to SMTP, which is the protocol to be used for e-mail transmission. At the time of e-mail transmission, this protocol executes authentication of the user account and the password between the SMTP server and the user to approve e-mail transmission only when it's authenticated.
NS-GSAPI | Limit GSSAPI auth method at SMTP auth
Lv.2 | Details | To restrict use of GSSAPI authentication method at the time of SMTP authentication.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: SMTP server-dependent, 1: Not used
Default value | 0
Supplement/memo | SMTP authentication: Protocol in which user authentication function is added to SMTP, which is the protocol to be used for e-mail transmission. At the time of e-mail transmission, this protocol executes authentication of the user account and the password between the SMTP server and the user to approve e-mail transmission only when it's authenticated.
NS-NTLM | Limit NTLM auth method at SMTP auth
Lv.2 | Details | To restrict use of NTLM authentication method at the time of SMTP authentication.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: SMTP server-dependent, 1: Not used
Default value | 0
Supplement/memo | SMTP authentication: Protocol in which user authentication function is added to SMTP, which is the protocol to be used for e-mail transmission. At the time of e-mail transmission, this protocol executes authentication of the user account and the password between the SMTP server and the user to approve e-mail transmission only when it's authenticated.
NS-PLNWS | Limit plaintext auth at SMTP auth encry
Lv.2 | Details | To restrict use of PLAIN/LOGIN authentication, which is plaintext, at the time of SMTP authentication under the environment where the communication packet is encrypted.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: SMTP server-dependent, 1: Not used
Default value | 0
Supplement/memo | SMTP authentication: Protocol in which user authentication function is added to SMTP, which is the protocol to be used for e-mail transmission. At the time of e-mail transmission, this protocol executes authentication of the user account and the password between the SMTP server and the user to approve e-mail transmission only when it's authenticated.
NS-PLN | Limit plaintext auth at SMTPauth noencry
Lv.2 | Details | To restrict use of PLAIN/LOGIN authentication, which is plaintext, at the time of SMTP authentication under the environment where the communication packet is not encrypted.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: SMTP server-dependent, 1: Not used
Default value | 0
NS-LGN | Limit LOGIN authentication at SMTP authentication
Lv.2 | Details | To restrict use of LOGIN authentication at the time of SMTP authentication.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: SMTP server-dependent, 1: Not used
Default value | 0
Supplement/memo | SMTP authentication: Protocol in which user authentication function is added to SMTP, which is the protocol to be used for e-mail transmission. At the time of e-mail transmission, this protocol executes authentication of the user account and the password between the SMTP server and the user to approve e-mail transmission only when it's authenticated.
MEAP-PN | HTTP port No.setting of MEAP application
Lv.2 | Details | To set HTTP port number of MEAP application.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Do not specify port 8080 when the Print Server is connected. Otherwise, you cannot browse the device RUI in which MEAP authentication application is running (Port 8080 is reserved for redirection of EFI Controller to the iR side.)
Display/adj/set range | 0 to 65535
Default value | 8000
SSH-SW | ON/OFF of SSH server function
Lv.2 | Details | To set ON/OFF of SSH server function.
Use case | As needed (This mode is used for the Japanese models only and not used with overseas models (outside Japan)).
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
Supplement/memo | SSH: Secure Shell. A program for logging into other PC through network, executing command from a remote PC, or moving files to other PC. Data on network is encrypted, so that a series of operation can be performed securely even through internet.
RMT-LGIN | Set to allow remote login to SSH server
Lv.2 | Details | To set whether to allow remote login from the remote host (SSH client: DA) to debug console of the SSH server.
Use case | As needed (This mode is used for the Japanese models only and not used with overseas models (outside Japan)).
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | This item is enabled when the setting value of SSH-SW is ON.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
Related service mode | COPIER> OPTION> NETWORK> SSH-SW (Level 2)
Supplement/memo | DA: Digital Accessory
RE-PKEY | Regeneration setting of SSH server key
Lv.2 | Details | To set whether to regenerate the SSH server pair key at the start of the machine. With the setting to regenerate the key, the SSH server host regenerates the pair key (private key/public key) at power-off/on, output to key file and store in HDD.
Use case | As needed (This mode is used for the Japanese models only and not used with overseas models (outside Japan)).
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - This item is enabled when the setting value of SSH-SW is ON. - Start of the machine might be approx. 3 to 4 minutes longer than the normal operation because regeneration process takes time.
Display/adj/set range | 0 to 1 0: Not regenerated, 1: Generated
Default value | 0
Related service mode | COPIER > OPTION > NETWORK > SSH-SW (Level 2)
U-NAME | Setting of SSH server login user name
Lv.2 | Details | To set the login user name which enables to connect to the SSH server. Only one user (host) is allowed to login.
Adj/set/operate method | 1) Select the item, and select the entry field. Keyboard is displayed. 2) Enter the character, and then press OK key.
Caution | This is active when COPIER> OPTION> NETWORK> SSH-SW is 1 (ON).
Display/adj/set range | 0 to 8 characters (1-byte alphanumeric characters)
Default value | gN3Fp2A
Related service mode | COPIER > OPTION > NETWORK > SSH-SW (Level 2)
U-PASWD | Set user password for SSH server connect
Lv.2 | Details | To set user password required for connecting to the SSH server. The entered characters are displayed as asterisks (*).
Adj/set/operate method | 1) Select the item, and select the entry field. Keyboard is displayed. 2) Enter the character, and then press OK key.
Caution | This is active when COPIER> OPTION> NETWORK> SSH-SW is 1 (ON).
Display/adj/set range | 0 to 8 characters (1-byte alphanumeric characters)
Default value | Vs8DuwJ (Asterisks (*) are displayed on the screen.)
Related service mode | COPIER > OPTION > NETWORK > SSH-SW (Level 2)
CHNG-STS | Set of TOT status connection port number
Lv.2 | Details | To set the port number for status connection with T.O.T.
Use case | When the Service NAVI is used
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 65535
Default value | 20010
Related service mode | COPIER> OPTION> NETWORK> STS-PORT
CHNG-CMD | Set of TOT command connection port No.
Lv.2 | Details | To set the port number for command connection with T.O.T.
Use case | When the Service NAVI is used
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 65535
Default value | 20000
Related service mode | COPIER> OPTION> NETWORK> CMD-PORT
MEAP-SSL | HTTPS port setting of MEAP
Lv.2 | Details | To set the port of HTTPS server in the case of using SSL with HTTP of MEAP.
Use case | When specifying the setting of HTTPS port for MEAP
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 65535
Default value | 8443
LPD-PORT | Setting of LPD port number
Lv.2 | Details | To set the LPD port number.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 65535
Default value | 515
Supplement/memo | LPD port: Network port for TCP/IP communication when making prints through network.
WUEV-SW | Setting of sleep notification execution
Lv.2 | Details | To set whether to notify the sleep mode to the application (imageWARE, etc) on the network when shifting to/recovering from the sleep mode.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Notified, 1: Not notified
Default value | 0
WUEV-INT | Setting of sleep notification interval
Lv.2 | Details | To set the interval of sleep notification.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | This is active when COPIER> OPTION> NETWORK> WUEV-SW is set to 0: Notified.
Display/adj/set range | 60 to 65535
Unit | 1 second
Default value | 600
Related service mode | COPIER> OPTION> NETWORK> WUEV-SW
WUEV-POT | Port number setting for sleep notice
Lv.2 | Details | To set port number of the PC to notify the sleep mode.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | This is active when COPIER> OPTION> NETWORK> WUEV-SW is set to 0: Notified.
Display/adj/set range | 1 to 65535
Default value | 11427
Related service mode | COPIER> OPTION> NETWORK> WUEV-SW
WUEV-RTR | Setting of sleep notification range
Lv.2 | Details | To set the number of available routers to the target for sleep notification.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | This is active when COPIER> OPTION> NETWORK> WUEV-SW is set to 0: Notified.
Display/adj/set range | 0 to 254
Default value | 3
Related service mode | COPIER> OPTION> NETWORK> WUEV-SW
WUEN-LIV | Recovery time setting after sleep notice
Lv.2 | Details | To set the time from the sleep start from network without job assignment until the mode is shifted to the sleep mode.
Use case | When setting the startup time after sleep notification
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 10 to 600
Unit | 1 second
Default value | 15
DHCP-12 | ON/OFF of DHCP-option 12 request
Lv.2 | Details | To set ON/OFF of inquiry on the host name (Option 12) which uses Option 55 of DHCP. Selecting OFF can prevent DHCP packet from including Option 12 or Option 81under the packet-monitoring network environment.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
Supplement/memo | DHCP: Dynamic Host Configuration Protocol
DHCP-81 | ON/OFF IPaddress dynamic chng in DHCP-81
Lv.2 | Details | To set ON/OFF for dynamic change of IP address by Option 81 of DHCP. Selecting OFF can prevent DHCP packet from including Option 12 or Option 81under the packet-monitoring network environment. Selecting ON enables dynamic change of IP address by Option 81 of DHCP in the case that the dynamic DNS setting is ON in user mode.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to set ON for the dynamic DNS setting in user mode to enable dynamic change of IP address.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
Supplement/memo | DHCP: Dynamic Host Configuration Protocol
IFX-CHIG | Set operation by IFAX recv mail content

Lv.1

Details

To set the number of characters for the IFAX received mail content, so that the mail is not printed/forwarded when the characters in the text is less than the number of specified characters.
This machine can output blank paper because some senders send e-mail text consists of linefeed codes only. In such case, specify 2 (number of characters) so that there will be no output of blank paper.
In the case of specifying any number other than 0, header/footer is printed/forwarded in 1 sheet only if the e-mail (body) text is less than the specified value while no TIFF file is attached.
As the value is incremented by 1, the number of target characters in e-mail body text is increased by 1 character.

Use case | When reducing print of blank paper due to e-mail received by IFAX
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to get approval from the user by telling that there will be no print of e-mail (body) text if the number of characters is less than the specified value.
Display/adj/set range | 0 to 999 0: E-mail (body) text is not ignored.
Unit | 1 character
Default value | 0
Supplement/memo | 1 Japanese Kanji character is calculated as 2 bytes, and the control codes (such as linefeed code, etc) are included in the number of characters.
DNSTRANS | Setting of DNS transfer priority
Lv.1 | Details | To set priority order of the protocol (IPv4/IPv6) to be used for DNS query. In the case of using both IPv6 and IPv4 while the DNS server supports IPv4, it takes time because of timeout when executing DNS query with priority on IPv6. Giving priority on query by IPv4 can shorten the time.
Use case | When it takes time to execute DNS query with priority on IPv6 because the DNS server supports IPv4
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: IPv4, 1: IPv6
Default value | 1
PROXYRES | Setting of proxy response to Windows
Lv.2 | Details | To set whether to provide proxy response or return the device status when an inquiry is received via Windows while the device is in sleep mode.
Use case | When executing status response for query from Windows correctly
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: No proxy response, 1: Proxy response
Default value | 1
WOLTRANS | Setting of sleep recovery protocol

Lv.1

Details

To set the protocol for recovery from sleep mode according to the value of WOL (Wake On LAN) trans.
Reception of a specific network packet is one of the requirements for the device to recover from sleep mode.
When the number of network protocols supported by the device increases, the types of network packets which activate recovery from sleep mode vary. However, there is a possibility that the existing network protocol is actually used.
Select the type of network packet which activates recovery from sleep mode according to the environment where the device is used.

Use case | When selecting protocol for sleep recovery
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 3 1: WSD and SNMP, 2: WSD and CPCA, 3: CPCA and SNMP
Default value | 1
TCPDLACK | Switch for the delay acknowledgment function
Lv.1 | Details | Select whether to enable/disable the delay acknowledge function. This item is used to disable the delay acknowledge function when the network data transfer performance level is decreased due to delay acknowledge in the 10M environment, etc.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 When this item is set to '0', the delay acknowledge function of TCP is disabled.
Default value | 1
802XTOUT | Set of IEEE802.1X authentication timeout
Lv.1 | Details | To set timeout value for IEEE802.1X authentication. If the device executes 802.1X authentication, change the wait time for response from the authentication server.
Use case | When response from the authentication server is slow/fast
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 10 to 120
Unit | second
Default value | 30
IKERETRY | Setting of IKE retry times
Lv.1 | Details | To set the number of retries in the case of no response from the communication target at the time of IKE packet transmission.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 3
Default value | 1
Supplement/memo | IKE: Internet Key Exchange
SPDALDEL | Initialization of SPD value
Lv.2 | Details | To initialize all the SPD values that are under management. SPD values can be initialized without clearing SRAM.
Use case | At the time of SPD value mismatch when IPSec Board is added
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
Supplement/memo | SPD: Database that manages SA (Security Association). SPD value is managed when IPSec Board is used. Normally, SRAM needs to be cleared in the case of mismatch in SPD value.
NCONF-SW | ON/OFF of Network Configurator function
Lv.1 | Details | To set ON/OFF of Network Configurator function. If the user does not use the function, select OFF to prevent remote attack through network.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
Supplement/memo | Network Configurator function is a function to be used for communication with NetSpot Device Installer, etc., and the network setting can be changed from the remote.
IKEINTVL | Setting of IKE retry interval
Lv.1 | Details | To set retry interval in the case of no response from the communication target at the time of IKE packet transmission.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 10
Unit | second
Default value | 5
Supplement/memo | IKE: Internet Key Exchange
IPSDEBLV | Setting of IPSec debug level
Lv.2 | Details | For R&D use
SP-LINK | Mode setting at 1W sleep
Lv.1 | Details | Switch to execute 10base-T standby as default to realize the standby power 1W in sleep mode.
Use case | When shifting to sleep mode after negotiation (same as conventional machines)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Shift to sleep mode with 10base-T 1: Shift to sleep mode after negotiation
Default value | 0
LM-LEVEL | Set of SMB client authentication method

Lv.1

Details

To set the authentication method (LM, NTLMv1, NTLMv2) that the SMB client uses for authentication.
In SMB authentication, authentication is generally made by the authentication method with higher level, and if it fails, the authentication level is lowered. (NLTMv2 => NLTMv1 => LM)
It is possible to limit the authentication level by setting 1 or 2 to avoid using the authentication method with lower level.

Use case | Upon user's request
Display/adj/set range | 0 to 2 0: Authentication is made by LM, NTLMv1 and NTLMv2 1: Authentication is made by NTLMv1 and NTLMv2 2: Authentication is made by NTLMv2
Default value | 0
Supplement/memo | Windows NT LAN Manager authentication: A user authentication method for network logon, which was generally used in the OS for Windows NT Series prior to Windows NT 4.0
AFS-JOB | Set of FAX server job reception port
Lv.1 | Details | To set the reception port of the fax server to which a fax client sends jobs.
Use case | When changing the job reception port of the fax server
Display/adj/set range | 0 to 65535
Default value | 20317
Related service mode | COPIER> OPTION> NETWORK> AFC-EVNT
AFC-EVNT | Set of FAX client event reception port
Lv.1 | Details | To set the event notification reception port of a fax client.
Use case | When changing the event notification reception port of a fax client
Display/adj/set range | 0 to 65535
Default value | 29400
Related service mode | COPIER> OPTION> NETWORK> AFS-JOB
ILOGMODE | Setting of IP address block mode
Lv.1 | Details | To set all protocols or TCP/UDP/ICMP unicast as the target of IP block. When 0 is set, the machine responds to ARP, ICMP multicast and broadcast which have no direct relation, and consequently the number of logs is increased. When 1 is set, the machine filters TCP, UDP and ICMP unicast only.
Use case | Upon user's request
Adj/set/operate method | 0 to 3 0: All protocols support mode 1: TCP/UDP/ICMP unicast support mode 2, 3: Not used
Default value | 0
ILOGKEEP | Set of IP address block log hold time
Lv.1 | Details | To set the retention time from the log time of IP block. When access is made again from a same IP address which was blocked before, if it is within the retention time of the previous log, its log is not recorded. If access is frequently made from a same IP address, the log record of the UI might be filled with its logs. If the user considers that a single log for a same IP address is enough, set the longer retention time.
Use case | Upon user's request
Display/adj/set range | 0 to 48 0: 1 minute (special mode) 1 to 48: 1 hour to 48 hours
Default value | 1
IPTBROAD | Set to allow broad/multicast TX

Lv.1

Details

To set whether to permit transmission of broadcast packets and multicast packets.
Transmission of broadcast packets and multicast packets is permitted without specifying an exception address. It is permitted within the device even if it is rejected in the default setting of the IPv4/v6 transmission filter.
Set ""1: Disabled"" when the user does not want to send them.

Use case | Upon user's request
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 5 0: Enabled, 1: Disabled, 2 to 5: Not used
Default value | 0
PFWFTPRT | Set of RST reply at IP filter FTP SEND

Lv.1

Details

When FTP SEND is executed using an IP filter by which packets from a specific remote PC are rejected, SYN is returned to the port 113 if the PC supports authentication of the FTP port 113. However, since the IP filter blocks the packets, the block logs are increased and the performance is lowered.
When 1 is set, RST is returned to the port 113 without blocking packets.

Use case | When executing FTP SEND against the OS which supports authentication of the FTP port 113 while the IP filter is enabled
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
PRNIPBLK | ON/OFF of IP address block function
Lv.1 | Details | To set ON/OFF of IP address block function. When 1 is set, ""IP Address Range Settings"" and ""RX/Print Range"" screen is displayed on the Control Panel.
Use case | When using the IP address block function
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | "0 to 1 0: OFF, 1: ON"
Default value | 0
Related user mode | Preferences> Network> TCP/IP Settings> IPv4 Settings/IPv6 Settings> IP Address Range Settings> RX/Print Range
IPMTU | Setting of MTU size
Lv.1 | Details | To set MTU size of network packet. This item is used when performing SEND communication between locations connected with Ethernet in a field environment where MTU black hole problem occurs.
Use case | When MTU black hole problem occur
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 1 to 10 1: 600 byte, 2: 700 byte, ..., 9: 1400 byte, 10: 1500 byte
Unit | 100 byte
Default value | 10
DDNSINTV | Set of DDNS periodical update interval
Lv.1 | Details | DNS registration is executed only once at start-up with the current iR, so the registered contents are deleted in an environment where the DNS server settings are deleted at intervals. To set the interval of DDNS periodical update for not deleting the registered contents.
Use case | When the DNS server settings are deleted at intervals
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 48 0: No periodical update, 1: 1-hour interval, 2: 2-hour interval, ..., 47: 47-hour interval, 48: 48-hour interval
Unit | 1 hour
Default value | 24