Installing the Printer Cover

| Print out this category

Installing the Printer Cover
1) Remove tapes on the printer cover.
2) The printer top front fover, the reader right cover and the reader left cover are secured with tapes.
3) Take out the cable of the printer outward.
4) Attach the printer top cover unit on the host machine.
Set the left stay with the bosses aligned.
Put the left stay of the host machine in the inside of the reader rear cover.
5) Fix the left stay.
2 Screws (Binding, M4×6)
6) Fix the printer top cover unit.
2 Screws (Binding, M4×6)
7) Remove the operation panel fixing plate from the bundled operation panel in the host machine.
2 Screw
8) Do it through the cales in the hole of the operation panel fixing plate .
9) Fix the operation panel fixing plate .
4 Screws (Binding, M4×6)
4 Screws (RS-tight, M3×8)
10) Route the cables as shown in the figure.
2 Wire saddles
11) Connet the 2 connectors to the operation panel.
1 Wire saddle
12) Attach the operation panel.
2 Screw (RS-tight, M3×8)
2 Claws
13) Install the reader right cover with the printer top cover slightly lifted.
3 Claws
2 Screw (RS-tight, M3×8)
CAUTION:
Be careful not to lift the printer top cover too high when installing the reader right cover.
14) Install the reader left cover with the printer top cover slightly lifted.
3 Claws
2 Screw (RS-tight, M3×8)
CAUTION:
Be careful not to lift the printer top cover too high when installing the reader left cover.
15) Install the printer top front cover.
2 Screw (RS-tight, M3×8)