CST-ADJ

| Print out this category

CST-ADJ

COPIER>ADJUST>CST-ADJ
MF-A4R | Adj of MP Tray A4R paper width
Lv.1 | Details | To adjust the width of A4R paper in the Multi-purpose Tray. When replacing the DC Controller PCB/clearing RAM data, enter the value of service label. When replacing the Multi-purpose Tray Paper Width Detection PCB or registering a new value, execute COPIER> FUNCTION> CST> A4R.
Use case | - When replacing the DC Controller PCB/clearing RAM data - When replacing the Multi-purpose Tray Paper Width Detection PCB or registering a new value
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 0 to 1024
Related service mode | COPIER> FUNCTION> CST> A4R
MF-A6R | Adj of MP Tray A6R paper width
Lv.1 | Details | To adjust the width of A6R paper in the Multi-purpose Tray. When replacing the DC Controller PCB/clearing RAM data, enter the value of service label. When replacing the Multi-purpose Tray Paper Width Detection PCB or registering a new value, execute COPIER> FUNCTION> CST> A6R.
Use case | - When replacing the DC Controller PCB/clearing RAM data - When replacing the Multi-purpose Tray Paper Width Detection PCB or registering a new value
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 0 to 1024
Related service mode | COPIER> FUNCTION> CST> A6R
MF-A4 | Adj of MP Tray A4 paper width
Lv.1 | Details | To adjust the width of A4 paper in the Multi-purpose Tray. When replacing the DC Controller PCB/clearing RAM data, enter the value of service label. When replacing the Multi-purpose Tray Paper Width Detection PCB or registering a new value, execute COPIER> FUNCTION> CST> A4.
Use case | - When replacing the DC Controller PCB/clearing RAM data - When replacing the Multi-purpose Tray Paper Width Detection PCB or registering a new value
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 0 to 1024
Related service mode | COPIER> FUNCTION> CST> A