﻿Paper Jam due to Solid Image Printed on Paper with Small Leading-Edge Margin (1-4 mm)

| Print out this category

Paper Jam due to Solid Image Printed on Paper with Small Leading-Edge Margin (1-4 mm)
[Occurrence area]
Fixing assembly
[Cause]
When a solid image is printed on the paper with a small leading-edge margin (1-4 mm), paper cannot be easily separated from the fixing film, causing a paper jam.
[Occurrence condition]
When the paper has been left alone in a high-humidity environment or when a solid image is printed on the paper with a small leading-edge margin.
[Remedy]
Service mode (Lv.2)> COPIER> OPTION> FEED-SW> SP-SW> 0 to 2
0: OFF
1: Separation priority mode 1 (Separation effect improves.)
2: Separation priority mode 2 (Separation effect improves more.)
Service mode (Lv.2)> COPIER> OPTION> IMG-FIX> TMP-TBLC> 0 to 3
0: Auto
1: OFF
2: N1 mode with plain paper 1/2 (Target temperature becomes low.)
3: N3 mode with plain paper 1/2 (Target temperature becomes moreover low.)