Measures in the Parts Replacement

| Print out this category

Measures in the Parts Replacement
When replacing the laser unit, enter the values recorded on the label affixed to the laser unit to be replaced for the following in the service mode:
Input example
Adjust of write start position of laser
A. (LV1) COPIER > ADJUST > LASER > PVE-OFST > 136
Difference in magnification between the lasers.
B. (LV1) COPIER > ADJUST > LASER > LDADJ1-K > -10
C. (LV1) COPIER > ADJUST > LASER > LDADJ2-K > 0
D. (LV1) COPIER > ADJUST > LASER > LDADJ3-K > 147
Difference in the phase between the lasers
E. (LV1) COPIER > ADJUST > LASER > LDADJ4-K > 93
F. (LV1) COPIER > ADJUST > LASER > LDADJ5-K > 16
G. (LV1) COPIER > ADJUST > LASER > LDADJ6-K > 117
NOTE:
There are two kinds of laser units of four beams (iRA4051/4045/4035) and two beams (iRA4025).
Changed the number of the pins of the connection connector as incompatible measures.