﻿Removing the Drum Unit

| Print out this category

Removing the Drum Unit
<Procedure>
1) Open the right cover.
2) Remove the waste toner container. (Reference)
3) Remove the screw securing the developing assembly pressure lever.
4) Turn the lever in the direction of the arrow to release the lock of the drum unit.
5) Pull out the drum unit slightly upward.
CAUTION:
Do not touch the drum surface during the work.
Cover the Drum Unit with paper not to expose the drum.
When inserting the drum unit, check that the drum unit is securely engaged with the rail of the host machine.