Network

| Print out this category

Network
If you are configuring the settings for the first time in "Interface Settings," "TCP/IPv4 Settings," "TCP/IPv6 Settings," or "Settings Common to TCP/IPv4 and TCP/IPv6," use the control panel of the machine. After configuring the TCP/IP settings, you can change them using the Remote UI.
In the NetWare or AppleTalk network, the TCP/IP protocol must be used to specify the settings with software other than the control panel of the machine. The setting items are shown below.
Some items can be set using the Remote UI. Use the control panel of the device to set items which cannot be set using the Remote UI.
* Default Settings
*1 Indicates items that appear only when the appropriate optional equipment is attached.
*2 Indicates items that appear only when the PS Printer Kit is activated.

Item | Setting Description | Can be set in Remote UI | Device Information Delivery Available
User Data List | Plint List | Yes | No
Confirm Network Connection Set. Changes | On, Off* | No | Yes
TCP/IP Settings
| IPv4 Settings
|  | Use IPv4 | On*, Off | Yes | No
|  | IP Address Settings | IP Address: 0.0.0.0* | Yes | No
|  | Subnet Mask: 0.0.0.0* | Yes | No
|  | Gateway Address: 0.0.0.0* | Yes | No
|  | DHCP: On, Off* | Yes | Yes
|  | RARP: On, Off* | Yes | Yes
|  | BOOTP: On, Off* | Yes | Yes
|  | PING Command | IP Adress: 0.0.0.0* | No | No
| IPv6 Settings | No
|  | Use IPv6 | On, Off* | Yes | No
|  | Stateless Address Settings | Use Stateless Address: On*, Off | Yes | No
|  | Manual Address Settings | Use Manual Address: On, Off* | Yes | No
|  | Manual Address: IPv6 Address (39characters maximum) | Yes | No
|  | Prefix Length: 0 to 128 (64*) | Yes | No
|  | Default Router Address (39 characters maximum) | Yes | No
|  | Use DHCPv6 | On, Off* | Yes | Yes
|  | PING Command | IPv6 Address: (39characters maximum) | Yes | No
|  | Host Name | 48 characters maximum | Yes | No
| DNS Settings
|  | DNS Server Address Settings
|  |  | IPv4 | Primary DNS Server: IP Address:0.0.0.0* | Yes | No
|  |  | Secondary DNS Server: IP Address:0.0.0.0* | Yes | No
|  |  | IPv6 | Primary DNS Server: IPv6 Address | Yes | No
|  |  | Secondary DNS Server: IPv6 Address | Yes | No
|  | DNS Host/Domain Name Settings |  | Yes | No
|  |  | IPv4 | Host Name: 47 characters maximum (Canon + represents the last six digits of a MAC address) | Yes | No
|  |  | Domain Name: 47 characters maximum | Yes | No
|  |  | IPv6 | Use Same Host Name/Domain Name as IPv4:On, Off* | Yes | No
|  |  | Host Name: 47 characters maximum (Canon + represents the last six digits of a MAC address) | Yes | No
|  |  | Domain Name: 47 characters maximum | Yes | No
|  | DNS Dynamic Update Settings
|  |  | IPv4 | DNS Dynamic Update: On, Off* | Yes | No
|  |  | IPv6 | DNS Dynamic Update: On, Off* | Yes | No
|  |  |  | Register Stateless Address: On, Off* | Yes | No
|  |  |  | Register Manual Address: On, Off* | Yes | No
|  |  |  | Register Stateless Address: On, Off* | Yes | No
| WINS Settings
|  | WINS Resolution | On, Off* | Yes | No
|  | WINS Server Address | IP Address: 0.0.0.0* | Yes | No
|  | Node Type | Auto Set, display only | No | No
|  | Scope ID | 63 characters maximum | Yes | No
| LPD Print Settings
|  | LPD Print Settings | On*, Off | Yes | Yes
|  | LPD Banner Page*1 | On, Off* | Yes | Yes
|  | RAW Print Settings |  |  |
|  |  | RAW Print Settings | On*, Off | Yes | Yes
|  |  | Bidirectional Communication | On, Off* | Yes | Yes
| SNTP Settings
|  | Use SNTP | On, Off* | Yes | No
|  | Polling Interval | Interval for performing time synchronization (1 to 48 hours) (24hours*) | Yes | No
|  | NTP Server Address | IP address or host name | Yes | No
|  | Check NTP Server | - | Yes | No
| FTP Print Settings
|  | Use FTP printing | On, Off* | Yes | Yes
|  | User | User name for FTP server login (24 characters maximum) | Yes | No
|  | Password | Password for FTP server login (24 characters maximum) | Yes | No
| WSD Print Settings
|  | Use WSD | On, Off* | Yes | Yes
|  | Use WSD Browsing | On, Off* | Yes | Yes
|  | Use Multicast Discovery | On, Off* | Yes | Yes
| Use FTP PASV Mode
|  | Use FTP PASV Mode | On, Off* | Yes | Yes
| IPP Print Settings
|  | IPP Print Settings | On, Off* | Yes | Yes
|  | Use SSL | On, Off* | Yes | No
|  | Use Authentication | On, Off* | Yes | No
|  | User | User name for IPP authentication (24 characters maximum) | Yes | No
|  | Password | Password for IPP authentication (24 characters maximum) | Yes | No
| Multicast Discovery Settings
|  | Response | On* Off | Yes | Yes
|  | Scope name | Scope name to be used for a multicast discovery (32 characters maximum) (default*) | Yes | No
| Use HTTP | On* Off | Yes | Yes
| Use Web DAV Server | On, Off* | Yes | Yes
| SSL Settings | Settings that use SSL | Yes | No
| Key and Certificate |  |  |
|  | Set as the Default Key | - | Yes | No
|  | Certificate Details | Version/Serial Number/Signature Algorithm/Issue Destination/Start Date of Validity/End Date of Validity/Issuer/Public Key/Cert Thumbprint/Certificate | Yes | No
|  | Display Use Location | Displays what the key pair is being used for | Yes | No
| Proxy Settings
|  | Use proxy | On, Off* | Yes | No
|  | Server Address | IP address or FQDN (128 characters maximum) | Yes | No
|  | Port Number | 1 to 65535 (80*) | Yes | No
|  | Use Proxy within the Same Domain | On, Off* | Yes | No
| Set Authentication
|  | Use Proxy Auth. | On, Off* | Yes | No
|  | User | 24 characters maximum | Yes | No
|  | Password | 24 characters maximum | Yes | No
| Confirm Dept. ID PIN | On, Off* | Yes | No
| IPSec Settings
|  | Use IPSec | On, Off* | Yes | No
|  | Receive Non-policy Packets | Allow*/Reject | Yes | No
|  | Edit |  | Yes | No
|  | Delete |  | Yes | No
|  | Policy On, Off |  | Yes | No
|  | Register |  |  |
|  |  | Policy Name | 24 characters maximum | Yes | No
|  |  | Register: Selector Settings | Local Address: All IP Addresses*/IPv4 Address/IPv6 Address/IPv4 Manual Settings/IPv6 Manual Settings | Yes | No
|  |  | Remort Address: All IP Addresses*, All IPv4Address, All IPv6Address, IPv4Manual Settings, IPv6 Manual Settings | Yes | No
|  |  | Port: Specify by Port Number*/Specify by Service Name | Yes | No
|  |  | IKE Settings | IKE mode : Main*/Aggressive | Yes | No
|  |  | Authentication Method : Pre-Shared Key Method*/Digital sig. Method | Yes | No
|  |  | Auth./Encryption Algorithm : Auto*/Manual Settings | Yes | No
|  |  | IPSec Network Settings | Validity : Time (1 to 65535minuites)(480minuites*) | Yes | No
|  |  | Validity : Size (1 to 65535 MB)(65535 MB*) | Yes | No
|  |  | PFS : On, Off* | Yes | No
|  |  | Auth./Encryption Algorithm : Auto*/Manual Settings | Yes | No
|  |  | Connect. Mode : Transport, display only | - | No
Netware Settings | Yes | No
| Use NetWare | On, Off* | Yes | Yes
| Frame Type | Auto Detect*/Ethernet II/Ethernet 802.2/Ethernet 802.3/Ethernet SNAP | Yes | No
| IPX External Network Number | Auto Set, display only | - | No
| Node Number | Auto Set, display only | - | No
| Print Service | Bindery PServer, R Printer, NDS Pserver*, NPrinter | Yes | No
| Packet Signature | Auto Set, display only | - | No
| Bindery Pserver Settings |  |  |
|  | Print Server Name | 47 characters maximum | Yes | No
|  | File Server Name | 47 characters maximum | Yes | No
|  | Print Server Password | 20 characters maximum | Yes | No
|  | Printer Number | 0 to 15 (0*) | Yes | No
|  | Polling Interval | 1 to 15seconds (5sedonds*) | Yes | No
|  | Printer Form | 0 to 255 (0*) | Yes | No
|  | Buffer Size | 1 to 20 KB (20KB*) | Yes | No
|  | Service Mode | Service only currently mounted form/Change forms as needed/Minimize form changes across print queues/Minimize form changes within print queues* | Yes | No
| Rprinter Settings
|  | Print ServerName | 47 characters maximum | Yes | No
|  | File ServerName | 47 characters maximum | Yes | No
|  | Printer Number | 0 to 15 (0*) | Yes | No
| NDS PServer Settings |  |  |
|  | Printer Number | 64 characters maximum | Yes | No
|  | Tree Name | 32 characters maximum | Yes | No
|  | Context | 256 characters maximum | Yes | No
|  | Print Server Password | 20 characters maximum | Yes | No
|  | Printer Number | 0 to 254 (0*) | Yes | No
|  | Polling Interval | 1 to 255 seconds (5seconds*) | Yes | No
|  | Printer Form | 0 to 255 (0*) | Yes | No
|  | Buffer Size | 3 to 20KB (20KB*) | Yes | No
|  | Service Mode | Service only currently mounted form/Change forms as needed/Minimize form changes across print queues/Minimize form changes within print queues* | Yes | No
| NPrinter Settings
|  | Print ServerName | 64 characters maximum | Yes | No
|  | Tree Name | 32 characters maximum | Yes | No
|  | Context | 256 characters maximum | Yes | No
|  | Printer Number | 0 to 254 (0*) | Yes | No
Apple Talk Settings
| Use Apple Talk | On, Off* | Yes | Yes
| Phase | Phase 2 (fixing) | - | No
| Service Name | 32 characters maximum (Model name*) | Yes | No
| Zone | 32 characters maximum | Yes | No
| Print Mode*2 | Both*, Spool, Direct | Yes | No
SMB Server Settings
| Use SMB Server | On, Off* | Yes | No
| ServerName | 15 characters maximum (Canon+represents the last six digits of a MAC address) | Yes | No
| Workgroup | 15 characters maximum (WORKGROUP*) | Yes | No
| Comment | 48 characters maximum | Yes | No
| LM Announce | On, Off* | Yes | No
| SMB Printer Settings |  |  |
|  | Use SMB Print | On, Off* | Yes | No
|  | Printer Name | 13 characters maximum (PRINTER*) | Yes | No
| SMB Auth. Settings |  |  |
|  | Use SMB Authentication | On, Off* | Yes | No
|  | Authentication Type | NTLMv1*, NTLMv2* | Yes | No
SNMP Settings | Yes | No
| Get Printer Mgmt Info from Host | On, Off* | Yes | Yes
| Use SNMPv1 | On*, Off | Yes | Yes
| Community Name1Settings |  |  |
|  | Community Name1 | On*, Off | Yes | No
|  | MIB Access Permission | Read/Write/Read Only* | Yes | No
|  | Community Name | Community Name (32 characters maximum) (public*) | Yes | No
| Community Name2 Settings |  | Yes | No
|  | Community Name2 | On, Off* | Yes | No
|  | MIB Access Permission | Read/Write/Read Only* | Yes | No
|  | Community Name | Community Name (32 characters maximum) (public2*) | Yes | No
|  | Use SNMPv3 | On, Off* | Yes | No
| User Settings
|  | User On, Off | - | Yes | No
|  | Register | User/MIB Access Permission/Security Settings/Authent.Algorithm/Authent.Password/Encryption Algorithm/Encryption Password | Yes | No
|  | Details/Edit | User/MIB Access Permission/Security Settings/Authent.Algorithm/Authent.Password/Encryption Algorithm/Encryption Password | Yes | No
|  | Delete | - | Yes | No
| Context Settings |  |  |
|  | Register | Context Name (32 characters maximum) | Yes | No
|  | Edit | Context Name (32 characters maximum) | Yes | No
|  | Delete | - | Yes | No
Dedicated Port Settings
| Dedicated Port Settings | On*, Off | Yes | Yes
Use Spool Function
| Use Spool Function | On, Off* | Yes | Yes
Startup Settings
| Startup Settings | 30 to 300 seconds (30*) | Yes | No
Ethernet Driver Settings
| Auto Detect | On*, Off | Yes | No
| Communication Mode | Half Duplex*/Full Duplex | Yes | No
| Ethernet Type | 10 Base-T*, 100 Base-TX, 1000 Base-T | Yes | No
| MAC Address | Display only | - | No
IEEE802.1X Settings
| Use IEEE802.1X | On, Off* | Yes | No
| Login Name | 24 characters maximum | Yes | No
| User | Name of the user to be authenticated with IEEE802.1X authentication | Yes | No
| Password | Password of the user to be authenticated with IEEE802.1X authentication | Yes | No
| TLS Settings
|  | Use TLS | On, Off* | Yes | No
| Key and Certificate
|  | Set as the Default Key | - | Yes | No
|  | Certificate Details | Version/Serial Number/Signature Algorithm/Issue Destination/Start Date of Validity/End Date of Validity/Issuer/Public Key/Cert.Thumbprint/Certificate | Yes | No
|  | Display Use Location | Displays what the key pair is being used for. | Yes | No
| TTLS Settings |  |  |
|  | Use TTL | On, Off* | Yes | No
|  | TTLS Settings | MSCHAPv2*, PAP | Yes | No
| PEAP Settings
|  | Use PEAP | On, Off* | Yes | No
|  | Same User Name as Login Name | On*, Off | Yes | No
Firewall Settings
| IP Address Block Log | Time, Category, IP Address, Result | Yes | No
| IPv4 Address Filter |  |  |
|  | TX Filter |  | Yes | No
|  |  | Use Filter | On, Off* | Yes | No
|  |  | Default Policy | Allow*/Reject | Yes | No
|  |  | IPv4 Address | Up to 16 IPv4 addresses can be stored. | Yes | No
|  | RX Filter |  |  |
|  |  | Use Filter | On, Off* | Yes | No
|  |  | Default Policy | Allow*/Reject | Yes | No
|  |  | IPv4 Address | Up to 16 IPv4 addresses can be stored. | Yes | No
| IPv6 Address Filter |  | Yes | No
|  | TX Filter |  |  |
|  |  | Use Filter | On, Off* | Yes | No
|  |  | Default Policy | Allow*/Reject | Yes | No
|  |  | IPv6 Address | Up to 16 IPv4 addresses can be stored. | Yes | No
|  | RX Filter |  |  |
|  |  | Use Filter | On, Off* | Yes | No
|  |  | Default Policy | Allow*/Reject | Yes | No
|  |  | IPv6 Address | Up to 16 IPv4 addresses can be stored. | Yes | No
| MAC Address Filter
|  | TX Filter
|  |  | Use Filter | On, Off* | Yes | No
|  |  | Default Policy | Allow*/Reject | Yes | No
|  |  | MAC Address | Up to 100 IPv4 addresses can be stored. | Yes | No
|  | RX Filter
|  |  | Use Filter | On, Off* | Yes | No
|  |  | Default Policy | Allow*/Reject | Yes | No
|  |  | MAC Address | Up to 100 IPv4 addresses can be stored. | Yes | No