Assembling the Option HDD

| Print out this category

Assembling the Option HDD
1) Assemble the option HDD.
CAUTION:
Be sure to use the Anti-vibration Damper included in HDD Mirroring Kit-F1 or HDD Data Encryption & Mirroring Kit-C4.
Never use the parts included in 2.5inch/80GB HDD-C1.
NOTE:
When tightening the screen, be sure to align the screw holes by lifting the HDD.
1 HDD Support Pate
4 Anti-vibration Damper (enclosed with HDD Mirroring Kit or HDD Data Encryption & Mirroring Kit.)
4 spacers
1 Option HDD
4 screws (binding with flat washer; M3X14)
CAUTION:
Assembling the option HDD, be careful of the installation direction.
Make sure that the label on the option HDD is facing up.
Make sure that [A] part of HDD Support Plate is placed at the opposite side of connector.