INSTALL

| Print out this category

FUNCTION
INSTALL

COPIER>FUNCTION>INSTALL
TONER-S | Toner supply to Developing Assembly
Lv.1 | Details | To execute a series of operation necessary for supplying toner to the Developing Assembly/Toner Supply area (drive the Developing Cylinder, Toner Stirring/Feed Member, Photosensitive Drum and ETB, and output developing bias) as a whole. After counting down from 600 seconds., it is stopped automatically.
Use case | - At installation - When replacing the Developing Assembly - When replacing toner in the Developing Assembly
Adj/set/operate method | 1) Select the items. ""Check the Developer"" is displayed. 2) Check connection, and then press OK key. It automatically stops after 10 minutes.
Caution | - Although ""Check the Developer"" is displayed when selecting the item, be sure to check the connection between the Developing Assembly and connector. - The operation can stop manually with OK key when a failure occurs.
Display/adj/set range | During operation: xxx second (remaining time), When operation finished normally: END
STRD-POS | Scan position auto adj in DADF mode
Lv.1 | Details | To adjust the DADF scanning position automatically.
Use case | At DADF installation/uninstallation
Adj/set/operate method | 1) Set a paper for stream reading position adjustment, and then close the DADF. 2) Select the item, and then press OK key. The operation automatically stops after the adjustment. 3) Write the value displayed by COPIER>ADJUST>ADJ-XY>STRD-POS in the service label.
Caution | Write the adjusted value in the service label.
Display/adj/set range | At normal termination: OK, At abnormal termination: NG
Required time | Approx. 10 seconds
Related service mode | COPIER> ADJUST> ADJ-XY> STRD-POS
Supplement/memo | For the details of paper for stream reading position adjustment, refer to the Service Manual.
CARD | Card number setting
Lv.1 | Details | To set the card number to be used for Card Reader. A series of numbers from the entered number to the number of cards specified by CARD-RNG can be used.
Use case | - At installation of the Card Reader - After replacement of the HDD
Adj/set/operate method | 1) Enter the number, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | The card management information (department ID and password) is initialized.
Display/adj/set range | 1 to 2001
Related service mode | COPIER> OPTION> FNC-SW> CARD-RNG (Level 2)
E-RDS | Set use/no use of Embedded-RDS function
Lv.1 | Details | To set whether to use the Embedded-RDS function.
Use case | When using Embedded-RDS
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to use E-RDS, RGW-PORT, COM-TEST, COM-LOG and RGW-ADR as a set.
Display/adj/set range | 0: Not used, 1: Used (All the counter information is sent.)
Related service mode | COPIER> FUNCTION> INSTALL> RGW-PORT, COM-TEST, COM-LOG, RGW-ADR
Supplement/memo | Embedded-RDS: Function to send device information such as the device counter, failure, and consumables to the sales company's server via SOAP protocol
RGW-PORT | Set port number of Sales Co's server
Lv.1 | Details | To set the port number of the sales company's server to be used for Embedded-RDS.
Use case | When using Embedded-RDS
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to use E-RDS, RGW-PORT, COM-TEST, COM-LOG and RGW-ADR as a set.
Display/adj/set range | 1 to 65535
Related service mode | COPIER> FUNCTION> INSTALL> E-RDS, COM-TEST, COM-LOG, RGW-ADR
Supplement/memo | Embedded-RDS: Function to send device information such as the device counter, failure, and consumables to the sales company's server via SOAP protocol
COM-TEST | Display connect result with the Sales Company's server
Lv.1 | Details | To display the result of the connection test with the sales company's server.
Use case | When using Embedded-RDS
Adj/set/operate method | Select the item, and then press OK key.
Caution | During operation: ACTIVE, When connection is completed: OK, When connection is failed: NG
Display/adj/set range | During operation: ACTIVE, When connection is completed: OK, When connection is failed: NG
Related service mode | COPIER> FUNCTION> INSTALL> E-RDS, RGW-PORT, COM-LOG, RGW-ADR
Supplement/memo | Embedded-RDS: Function to send device information such as the device counter, failure, and consumables to the sales company's server via SOAP protocol
COM-LOG | Display connect error with the Sales Co's server
Lv.1 | Details | To display error information when the connection with the sales company's server failed.
Use case | When using Embedded-RDS
Adj/set/operate method | Display only
Caution | Be sure to use E-RDS, RGW-PORT, COM-TEST, COM-LOG and RGW-ADR as a set.
Display/adj/set range | Year, date, time, error code, error detail information (maximum 128 characters)
Related service mode | COPIER> FUNCTION> INSTALL> E-RDS, RGW-PORT, COM-TEST, RGW-ADR
Supplement/memo | Embedded-RDS: Function to send device information such as the device counter, failure, and consumables to the sales company's server via SOAP protocol
RGW-ADR | URL setting of Sales Company's server
Lv.1 | Details | To set the URL of the sales company's server to be used for Embedded-RDS.
Use case | When using Embedded-RDS
Adj/set/operate method | 1) Select the URL. 2) Enter the URL, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Do not use Shift-JIS character strings. - Be sure to use E-RDS, RGW-PORT, COM-TEST, COM-LOG and RGW-ADR as a set.
Display/adj/set range | URL
Related service mode | COPIER> FUNCTION> INSTALL> E-RDS, RGW-PORT, COM-TEST, COM-LOG
Supplement/memo | Embedded-RDS: Function to send device information such as the device counter, failure, and consumables to the sales company's server via SOAP protocol
CNT-DATE | Set counter send start date to sales company's server
Lv.1 | Details | To set the year, month, date, hour and minute to send counter information to the sales company's server. This is displayed only when the Embedded-RDS third-party extended function is available.
Use case | When the Embedded-RDS third-party expanded function is available
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | YYYYMMDDHHMM (12 digits) YYYY: Year, MM: Month, DD: Date, HH: Hour, MM: Minute
Supplement/memo | Embedded-RDS: Function to send device information such as the device counter, failure, and consumables to the sales company's server via SOAP protocol
CNT-INTV | Set counter send interval to the sales company's server
Lv.1 | Details | To set the interval of sending counter information to the sales company's server in a unit of one hour. This is displayed only when the Embedded-RDS third-party extended function is available.
Use case | - When restarting potential control after execution of COPIER> OPTION> IMG-FIX> PO-CNT - When the D-max control condition is changed
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 168 (=1 week)
Unit | 1 hour
Supplement/memo | Embedded-RDS: Function to send device information such as the device counter, failure, and consumables to the sales company's server via SOAP protocol
BRWS-ACT | ON/OFF of service browser
Lv.1 | Details | To set whether to set ON/OFF of the browser for servicing. When 2 is specified, the browser becomes enabled temporarily. This mode can be used when checking operation.
Use case | - When using the browser for servicing - At operation check
CDS-CTL | Set country/area when using CDS
Lv.1 | Details | To set country/area to enable CDS.
Use case | When enabling CDS
Display/adj/set range | Country/area set in COPIER> OPTION> FNC-SW> CONFIG, CA (Canada), LA (Latin America) and HK (Hong Kong)
Related service mode | COPIER> OPTION> FNC-SW> CONFIG
Supplement/memo | CDS: Contents Delivery System
DRM-INIT | Initialization of Photosensitive Drum
Lv.1 | Details | To initialize Photosensitive Drum. Clear drum counter (DRM-CNTR), Drum Lot number, and checksum stored in the DC Controller.
Use case | After replacement of the Photosensitive Drum
Adj/set/operate method | Select the item, and then press OK key.
Display/adj/set range | During operation: ACTIVE, At normal termination: OK, At abnormal termination: NG
Related service mode | COPIER> COUNTER> MISC> DRM-CNTR