CLEAR

| Print out this category

CLEAR

COPIER>FUNCTION>CLEAR
ERR | Clear of error code
Lv.1 | Details | To clear error codes (E000, E001, E002, E003, E717, E719). E000, E001, E002, and E003 are fixing-related errors. E004 (IH Power Supply) and E005 (Web absence) do not need to be cleared.
Use case | At error occurrence
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
DC-CON | RAM clear of DC Controller PCB
Lv.1 | Details | To clear the RAM data of the DC Controller PCB.
Use case | When clearing the RAM data of the DC Controller PCB
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Output the service mode setting values by P-PRINT before execution. After execution, enter necessary setting values. - The RAM data is cleared after the main power switch is turned OFF/ON.
Related service mode | COPIER> FUNCTION> MISC-P> P-PRINT
R-CON | RAM clear of CCD unit (CCD PCB)
Lv.1 | Details | To clear the RAM data of the CCD unit (CCD PCB).
Use case | When clearing the RAM data of the CCD unit (CCD PCB)
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Output the service mode setting values by P-PRINT before execution. After execution, enter necessary setting values. - The RAM data is cleared after the main power switch is turned OFF/ON.
Related service mode | COPIER> FUNCTION> MISC-P> P-PRINT
JAM-HIST | Clear of jam history
Lv.1 | Details | To clear the jam history.
Use case | When clearing the jam history
Adj/set/operate method | Select the item, and then press OK key.
Related service mode | COPIER> DISPLAY> JAM
ERR-HIST | Clear of error code history
Lv.1 | Details | To clear the error code history.
Use case | When clearing the error code history
Adj/set/operate method | Select the item, and then press OK key.
Related service mode | COPIER> DISPLAY> ERR
PWD-CLR | Clear of system administrator password
Lv.1 | Details | To clear the password of the system administrator set in the user mode.
Use case | When clearing the password of the system administrator
Adj/set/operate method | Select the item, and then press OK key.
ADRS-BK | Clear of address book
Lv.1 | Details | To clear the address book data.
Use case | When clearing the address book data
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | The address book data is cleared after the main power switch is turned OFF/ON.
CNT-MCON | Clear of Main Controller service counter
Lv.1 | Details | To clear the service counter counted by the Main Controller PCB.
Use case | When clearing the service counter counted by the Main Controller PCB
Adj/set/operate method | Select the item, and then press OK key.
Related service mode | COPIER> COUNTER
Supplement/memo | See COUNTER for the target counter.
CNT-DCON | Clear of DC Controller service counter
Lv.1 | Details | To clear the service counter counted by the DC Controller PCB.
Use case | When clearing the service counter counted by the DC Controller PCB
Adj/set/operate method | Select the item, and then press OK key.
Related service mode | COPIER> COUNTER
OPTION | Clear of service mode setting value(OPTION)
Lv.1 | Details | To return the value specified in service mode (OPTION) to the default value (value at the time of RAM clear).
Adj/set/operate method | Select the item, and then press OK key.
Caution | - Output the service mode setting values by P-PRINT before execution. After execution, enter necessary setting values. - This item is executed for the data on the Main Controller PCB, DC Controller PCB and CCD unit (CCD PCB).
Related service mode | COPIER> FUNCTION> MISC-P> P-PRINT
MMI | Clear of user mode setting value

Lv.1

Details

To clear the user mode setting values (excluding values for Control Panel, common settings, and FAX).
- Common Settings
- Timer Settings
- Adjustment/Cleaning
- Report Settings
- System Settings
- Copy Settings
- Communications Settings
- Printer Settings

Use case | When clearing various setting values of user mode
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | The setting value is cleared after the main power switch is turned OFF/ON.
MN-CON | RAM clear of Main Controller PCB SRAM Board
Lv.1 | Details | To clear the RAM data of the Main Controller PCB SRAM Board. All data on the SRAM Board is initialized.
Use case | When clearing the RAM data of the Main Controller PCB SRAM Board
Adj/set/operate method | 1) Select the item, and then press OK key. The machine is automatically rebooted. 2) Turn OFF/ON the main power switch.

Caution

- Address Book, Forwarding Settings, Settings/Registration (Preferences), Adjustment/Maintenance, Function Settings, Set Destination, management
- Inform the user that all images in Inbox will be deleted and get approval for it.
- Since the file management information is initialized, images on the HDD cannot be read.
- Output the service mode setting values by P-PRINT before execution. After execution, enter necessary setting values.
- the RAM data is cleared After the main power switch is turned OFF/ON.

Related service mode | COPIER> FUNCTION> MISC-P> P-PRINT
CARD | Clear of card ID-related data
Lv.1 | Details | To clear the data related to the card ID (department).
Use case | When clearing the data related to the card ID
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | The value is cleared after the main power switch is turned OFF/ON.
ALARM | Clear of alarm log
Lv.1 | Details | To clear alarm log.
Use case | When clearing alarm log
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | The alarm log is cleared after the main power switch is turned OFF/ON.
Related service mode | COPIER> DISPLAY> ALARM-2
CA-KEY | Deletion of CA certificate and key pair
Lv.1 | Details | To simultaneously delete the CA certificate and key pair which are additionally registered by the user.
Use case | When a service person replaces/discards the device
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Check that OK is displayed. 3) Turn OFF/ON the main power switch.

Caution

- Unless this item is executed at the time of replacement/discard of the device, the CA certificate and key pair which are additionally registered by the user remain in the HDD, which is a problem in terms of security.
- Do not execute this item carelessly because the CA certificate and key pair which are additionally registered are deleted when it is executed. If they are deleted mistakenly, they need to be again registered by the user. If no CA certificate and key pair are additionally registered, the machine condition becomes the same as the one at the time of factory shipment.
- When NG is displayed in 2), there is a possibility that deletion was not executed. In this case, surely execute the deletion by initializing the HDD, etc.

Supplement/memo | - The CA certificate is used in the MEAP application with E-RDS and SSL client connection, and the key pair is used in the SSL function of IPP, RUI and MEAP. - When the main power switch is turned OFF/ON, the CA certificate and key pair which were registered at the time of factory shipment are decompressed from the archive (/BOOTDEV/KCMNG), and become available in the E-RDS/SSL function.
ERDS-DAT | Initialization of E-RDS SRAM data
Lv.1 | Details | To initialize the SCM value of the Embedded-RDS stored in the SRAM. SCM values are ON/OFF of E-RDS, server's port number, server's SOAP URL, and communication schedule with the server (how often the data is acquired), etc. The value set by COPIER> FUNCTION> INSTALL> E-RDS, RGW-PORT, RGW-ADR, COM-LOG is cleared.
Use case | When upgrading the Bootable in the E-RDS environment
Adj/set/operate method | Select the item, and then press OK key.
Caution | The method of using the SRAM in E-RDS differs depending on the Bootable version. Therefore, unless the SRAM data is cleared at the time of version upgrade, data inconsistency occurs.
Related service mode | COPIER> FUNCTION> INSTALL> E-RDS, RGW-PORT, RGW-ADR, COM-LOG
KEY-CLR | Encrypt key clear of HDD Encrypt Board
Lv.1 | Details | To clear the encryption key of the HDD Encryption Board (Security Kit) for replacement. Processing is executed at the time of replacement of the Encryption Board, and a new encryption key is generated.
Use case | When replacing the encryption key for the HDD Encryption Board
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Check that OK is displayed. 2) Turn OFF/ON the main power switch.
Caution | Since all data in the HDD becomes unavailable when executing this item, be sure to initialize the HDD after turning OFF/ON the main power switch.
USBM-CLR | Initialize USB MEAP priority registration info
Lv.1 | Details | To initialize the registered ID data retained in the OS field by calling the API provided by the OS.
Use case | When a failure occurs in USB MEAP priority registration
JV-CACHE | Cache clear of JAVA application
Lv.1 | Details | To clear the cache information used by JAVA application.
Use case | When initializing the JAVA application
Adj/set/operate method | Select the item, and then press OK key.
FXTX-CLR | Clearing fax job information
Lv.1 | Details | To clear fax job information stored on SRAM. Use this mode to restore from E611-0001.
Use case | When E611-0001 occurs
Adj/set/operate method | Select the item, and then press OK key.
LANG-CLR | Uninstallation of local language:Java UI
Lv.1 | Details | To uninstall the local language (Java UI). If this mode is executed, the language files other than English and Japanese are deleted. Screen is displayed in English.
Use case | When uninstalling the local language
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Reboot the machine.