Installation to the Host Machine

| Print out this category

Installation to the Host Machine
1) Install the HDD Face Plate to the HDD Box.
2 Screws (TP Round End; M3X6)
CAUTION:
Be sure to use the round end screw included in the Removable HDD Kit as the TP screw.
2) Install the HDD Door Unit to the HDD Box.
1 Boss
1 HDD Lock Plate Shaft
1 Hinge Shaft Stopper
3) Remove the plate from the HDD Box. (The removed plate will not be used.)
1 Screw (The removed screw will be used in step 5.)
4) Disconnect the 2 Drawer Cables of the HDD Drawer Unit, and replace them with the IV cables. (The removed 2 Drawer Cables will not be used.)
4 Screws (Use the 2 screws. The remaining 2 screws will not be used.)
4 Springs (Use the 2 springs. The remaining 2 springs will not be used.)
4 Washers (Use the 2 washers. The remaining 2 washers will not be used.)
5) Install the HDD Drawer Unit.
1 Screw (Use the screw removed in step 3.)
6) Install the HDD Box to the HDD Slide Rail.
4 Claws
4 Screws (Use the 4 screws removed in ”Removing the HDD" step 9.)
7) Put the 2 cables through, and return the HDD Unit to the host machine.
NOTE:
Be sure to move the unit in the direction of the arrow when installing it to prevent the protrusion of the HDD Slide Rail from coming in contact with the plate of the host machine.
Be sure not to push the cable in the host machine.
8) Disconnect the 2 cables on the Controller side. (The 2 removed cables will not be used.)
2 Connectors
3 Edge Saddles
2 Wire Saddles
9) Connect the 2 cables of the HDD Unit.
2 Connectors
3 Edge Saddles
3 Wire Saddles
NOTE:
Be sure to pass the cable through the Wire Saddle [A] when connecting.
10) Secure the HDD Unit.
2 Screws (Use the screws removed in "Removing the HDD" step 8.)
CAUTION:
Be careful not to drop the screw.
Be sure to tighten the screws in the order shown in the figure.
11) Close the plate.
12) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
13) Connect the USB Cable and the Control Panel Communication Cable.
14) Install the covers.
Controller Box Cover
Rear Cover (4 Screws) (Tighten the screws in the following order: upper left, lower left, upper right, and then lower right.)
Right Rear Cover (2 Screws)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.
15) pen the Small Cover of the Right Rear Cover, and affix the label.
1 Shutdown Cuution Label
16) Open the HDD Door Unit.
17) Install the Removable HDD 1 (front).
NOTE:
Be sure to insert it until it stops.
18) Close the HDD Door Unit.
19) Be sure to request the user to padlock the removable HDD to discourage theft.
20) Close the Small Cover of the Right Rear Cover.