Steps to Service Browser settings

| Print out this category

Steps to Service Browser settings
1. Start [Service Mode] at Level 1.
For the procedures, see “Steps to E-RDS settings - step 1.“.
2. Select [COPIER] > [Function] > [INSTALL] > [BRWS-ACT] and then touch [OK].
NOTE:
E-RDS sends browser information to UGW at this timing.
If the connection is established with UGW successfully, “OK!” is displayed. When “NG!” is displayed, perform the steps referring to “Troubleshooting” until connection is established with UGW.
3. Reboot the device.
4. Make sure that “1 (: ACTIVE)” is set under [COPIER] > [Display] > [USER] > [BRWS-STS].
5. When the above-shown setting values are enabled, [Service Browser] is displayed in the Service Mode screen.