PASCAL Control

| Print out this category

PASCAL Control
This control stabilizes gradation density characteristics on the image.
This control is executed when the following is selected in user mode: Auto Adjust Gradation >
Full Adjust
Patch pattern on the test print is scanned by the Reader to create a gradation table
(PASCALγLUT).
Execution timing
During execution of Full Adjust: User mode > Settings/Registration > Adjustment/Maintenance
> Adjust Image Quality > Auto Adjust Gradation