CLEANING

| Print out this category

CLEANING

COPIER>OPTION>CLEANING
FX-CN-SW | Set fix pressure roller cln sequence
Lv.2 | Details | To set the fixing pressure roller cleaning sequence
Use case | Upon user's request (When the fixing motor sound which is generated in the cleaning sequence is claimed from user)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 1