Service mode menu Transmission﻿

| Print out this category

Service mode menu Transmission﻿
E-RDS sends the target service mode menu data to UGW in the following cases:
When a specific alarm and service call error are detected
When the setting is changed in service mode
The following shows the transmission timing and the target data for transmission in service mode menu:

Transmission timing | Transmitting data | Error retry

When the following alarm is detected.
Alarm codes for transmission:
0x060002,                     // Fixing
0x060004 - 0x069999,  // Fixing
0x090005 - 0x099999,  // Dram
0x100006 - 0x109999,  // Development
0x300001 - 0x309999   // High voltage

COPIER

Display

ANALOG

No

HV-STS
CCD
DPOT
DENS
FIXING
SENSOR
MISC
HT-C
HV-TR
P-PASCAL
When the following service call error is detected. Error codes for transmission: E000 - E00F,  // Fixing E020,              // Development ATR E060 - E06F   // High voltage | COPIER | Display | ANALOG | No
HV-STS
CCD
DPOT
DENS
FIXING
SENSOR
MISC
HT-C
HV-TR
P-PASCAL
When a value is set to [COPIER - Adjust] subordinate’s Service mode menu. (Transmission will be done at 60 min, later of setting) | COPIER | Adjust | Yes
When the first communication test is done. (For transmission process, 5 minutes after the execution) | COPIER | Display | ANALOG | Yes
HV-STS
CCD
DPOT
DENS
FIXING
SENSOR
MISC
HT-C
HV-TR
P-PASCAL
Adjust

NOTE:
Target transmission data are only the items under LEVEL1 and 2 in the service mode.