IMG-MCON

| Print out this category

IMG-MCON

COPIER>OPTION>IMG-MCON
PASCAL | Use/no use of auto gradation adj data
Lv.1 | Details | To set to use/not to use the gradation adjustment data gamma LUT that is generated by auto gradation adjustment (Full/Quick Adjust) control. Selection is available as to whether to use gamma LUT at the time of image formation.
Use case | When PASCAL-related failure occurs/when identifying the cause of PASCAL-related failure
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 3 0: Initial LUT is used. (Automatic gradation adjustment is not used.) 1: Auto gradation adjustment is used. 2 to 3: Not used
Default value | 1
SHARP | Setting of sharpness level of image
Lv.2 | Details | To set the setting level (center value) of sharpness of image. As the value is increased, the image tends to be sharp, and as the value is decreased, image tends to be soft.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 5
Default value | 3
VP-ART | Setting of line art processing

Lv.2

Details

To set outline processing for line art on scalable PDF.
In the outline processing, a binary image outline is extracted in the field which is recognized as line art, and is converted into vector data.
Specify whether to convert the binary image outline into vector data or to recognize it as one line (as a thin line). For the thin line, the line width can be specified.
Change this value when you want to obtain an output of a wide-width line as one line rather than as an outline (when you want to prioritize edit operation as a line rather than image quality).

Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 99
Default value | 1
VP-TXT | Setting of character vectorization

Lv.2

Details

To set vector conversion processing for text on scalable PDF.
In the vector conversion processing, a binary image outline is extracted in the field which is recognized as text, and is converted into vector data.
In regular vector conversion, function approximation is not used for small text because the image quality is not changed.
When the value is changed, function approximation processing is executed for small text, which realizes smooth text although the image quality is changed.
Change this value when you want to prioritize smoothness in small text.

Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 99
Default value | 1
LIN-OFST | Set special paper added dot amnt offset

Lv.1

Details

To set the offset amount of dots added to vertical/horizontal direction when lines on special paper are thinner than those on plain paper.
When printing special paper, compared to plain paper, the amount of dots specified with this item is added.
As the value is larger, lines become thicker.
When WDREDUCT is 0, this setting is enabled.

Use case | When the line width of special paper is thinner than the one of plain paper
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 4
Default value | 1