Work Procedure

| Print out this category

Work Procedure
Device Setting Procedure
1) Start [ SERVICE MODE ] in Level 1.
2) Press [ COPIER ] > [ Option ] > [ DSPLY-SW ] buttons.
3) Press [ RMT-CNSL] button.
4) Press either 1 (activate remote console function) on control panel (the numerical value input in the field is displayed), and press [ OK ] button.
5) Check to see that it is reflected in setting field, and restart the device.
PC setting procedure (when Tera Term is used)
1) Install the terminal software on the PC.
2) Start the terminal software, make the following settings, and then click the "OK" button.

Connection | : Select [TCP/IP] (Default)
Host | : Device Host Name or IP Address
Service | : Select "Telnet"
TCP port# | : Enter 19001

3) The connection window will open. Select [Terminal…] from the [Setup] menu.
4) The terminal setting screen will appear. Make the following settings, and then click the "OK" button.

Terminal ID | : VT100
New-line Receive | : LF

5) Select [Log...] from the [File] menu.
6) The dialog for specifying the save destination of the log file will appear. Set the save destination path and the file name, and then click the [Save] button.
7) Perform the operation whose log you want to collect.
8) Click the [Close] button in the log dialog.
Note:
To suspend log collection, click the [Pause] button.
Note:
While collecting logs, the following operations are available from the [File] menu.
Comment to Log... :
You can add a comment to the log being collected. The added comment is reflected in the log file.
Show Log dialog... :
The logs that have been collected are pasted on Notepad and displayed.
Change directory... :
The preliminarily set save destination of the log file can be changed.
9) Open the file saved in the save destination, and check that the logs are stored correctly.
Note:
Depending on the MEAP application, the log output setting needs to be made in order to collect logs.
CAUTION:
After collecting logs, the remote console function of the device needs to be disabled (select [SERVICE MODE] LEVEL1 > [COPIER] > [Option] > [DSPLY-SW] > [RMT-CNSL] > 0, and restart the device).
PC setting procedure (when Hyper Terminal is used)
1) Start Hyper Terminal, set the connection name in the [Connect Description] dialog that appears on the screen, and then click the OK button.
2) Set [TCP/IP(Winsock)] for [Connect using].
3) Enter the IP address of the target device in [Host address], and enter "19001" (fixed) in [Port number].
4) Click the "Properties" icon on the Hyper Terminal screen.
5) The [Console Properties] dialog will appear. Select the [Settings] tab, select [VT100] for [Emulation], and then click the [OK] button.
6) Return to the Hyper Terminal window, and select [Transfer] > [Capture Text...] from the menu.
7) The dialog for specifying the save destination of the log file will appear. Specify the save destination.
8) Perform the operation whose log you want to collect.
9) Select [Transfer] > [Capture Text...] > [Stop] from the menu.
10) Open the file saved in the save destination, and check that the logs are stored correctly.
Note:
Depending on the MEAP application, the log output setting needs to be made in order to collect logs.
CAUTION:
After collecting logs, the remote console function of the device needs to be disabled (select [SERVICE MODE] LEVEL1 > [COPIER] > [Option] > [DSPLY-SW] > [RMT-CNSL] > 0, and restart the device).