External 2, 2/3, 2/4, 4 Hole Puncher-B2 SORTER > P032 to P037

| Print out this category

External 2, 2/3, 2/4, 4 Hole Puncher-B2 SORTER > P032 to P037

Address | bit | Name | Symbol | Remarks
PORT32 | 7 | Punch HP sensor | PI63 | 0: HP
6 | For R&D use |  |
5 | Rear End Detector Sensor | PCB11/12 | 1:Paper presence (LED5,PTR5)
4 | For R&D use |  |
3 | Not used |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT33 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT34 | 7 | Punch Motor Direction Change Signal (CW) | M61 | 0: ON
6 | Punch Motor Direction Change Signal (CWW) | M61 | 0: ON
5 | Horizontal Registration Motor Standby | M62 | 0: Standby
4 | Horizontal Registration HP Sensor | PI61 | 1: HP
3 | For R&D use |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | For R&D use |  |
PORT35 | 7 | Not used |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
PORT36 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | Front Door Switch | MSW62 | 0:open
3 | For R&D use |  |
2 | Horizontal Registration Motor B | M62 | 0:Phase B* ON, 1:Phase B ON
1 | Horizontal Registration Motor A | M62 | 0:Phase A* ON, 1:Phase A ON
0 | For R&D use |  |
PORT37 | 7 | A3 Horizontal Registration Sensor | PCB11/12 | 0:Paper presence (LED1,PTR1)
6 | Scrap Full Detector Sensor | PCB13 | 0:Paper presence (LED6,PTR6)
5 | Upper Door Switch | MSW61 | 0:Open
4 | Not used |  |
3 | B4 Horizontal Registration Sensor | PCB11/12 | 0:Paper presence (LED2,PTR2)
2 | A4R Horizontal Registration Sensor | PCB11/12 | 0:Paper presence (LED3,PTR3)
1 | B5R Horizontal Registration Sensor | PCB11/12 | 0:Paper presence (LED4,PTR4)
0 | Not used |  |