DENS

| Print out this category

DENS

COPIER>ADJUST>DENS
DENS-ADJ | Density correction of copy image
Lv.1 | Details | To correct the density of copy image by changing the F-value table. When replacing the DC Controller PCB/clearing RAM data, enter the value of service label. Blurring is alleviated when the value is increased, and fogging is alleviated when the value is decreased.
Use case | When fogging or blurring at high density area occurs with a copy image
Adj/set/operate method | Enter the setting value, and then press OK key.
Caution | Density of printer output image cannot be corrected.
Display/adj/set range | 1 to 9
Appropriate target value | 4 to 6
Default value | 5