Installation Procedure

| Print out this category

Installation Procedure
1) Remove the Right Rear Cover (Upper).
2 Screws
2 Protrusions
1 Claw
2) Disconnect the USB Cable and the Control Panel Communication Cable.
3) Remove the Main Controller PCB 1.
2 Screws (beside of arrow mark)
1 Connector
CAUTION:
Be sure to move the USB Cable and the Control Panel Communication Cable to the Reader side to prevent the cables from being trapped.
CAUTION:
Be sure to place the removed Main Controller PCB 1 on flat surface.
Reason: Since the fan protrudes, if it is placed at a tilt, it may be damaged.
4) Remove the Screw and the Spacer from the Voice Guidance Board Unit. (The removed screw and spacer will not be used.)
5) Remove the Face Plate from the Main Controller PCB 1 . (The removed Face Plate will not be used.)
6) Install the Voice Guidance Board Unit.
1 Connector
4 Screws (TP; M3x6)
NOTE:
Check that the connector is connected properly.
7) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
8) Install the USB Cable and Control Panel Communication Cable.
9) Remove the screw and the Face Seal from the Reader Right Cover.
1 Screw (The removed screw will not be used.)
1 Face Seal (The removed Face Seal will not be used.)
10) Install the Speaker Unit (Lower).
1 Screw (Binding; M3x16)
1 Screw (Binding; M4x16)
11) Install the Speaker Unit (Upper).
1 Screw (Binding; M4x6)
12) Install the Ring Cores to both ends of the Speaker Cable.
13) Connect the Speaker Cable to 2 points.
14) Cut off [A] part of the Right Upper Sub Cover with nippers.
NOTE:
When cutting off the part, be sure not to make burrs.
15) Put the Speaker Cable through the cut-off of the Right Cover (Upper Rear), and return the cover to its original position.
2 Screws (Use the screws removed in step 1.)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.
16) Remove the covers of 4 Cord Guides.
17) Remove the release paper from the Cord Guides, and affix the guides to the 4 areas indicated in the figure.
18) Put the Speaker Cable through the Cord Guides and install the covers of the guides.
NOTE:
When installing the Card Reader simultaneously, affix a Cord Guide to the area indicated in the figure.