Preconditions:

| Print out this category

Preconditions:
The log is stored in the machine by holding down the counter + 1.2.3 or the automatic log collection function.
A PC with SST running is connected to the machine and the machine is at download mode by starting it with the 2 and 8 keys.
Note:
Executing a log collection by SST deletes logs in the machine.
1. Start SST (Ver. 4.41 or later) and select iRC5051 from Model List. Press the Start button.
2. Press the Upload Data button.
3. Select the data to be uploaded, then click [Start] button.
When there is no log in the machine, it results in blank option items for "data to upload".
When the file name is longer than the frame, it displays that it is a log in the comment column just below.
It is displayed as "log" in the figure below.
Note:
The log is not stored when You cancel it before pushing the Start button.
It is deleted from the main body.
4. Press the "Save" button.
5. Check that the data storage is completed and click the "OK" button.
6. Check that the log is stored in the specified location in the PC.
In the initial setting:
Windows(C:) > ServData > iRC5051 >EXR02627 (Serial number)