Required Options and Conditions

| Print out this category

Function Expansion System Options
Required Options and Conditions
Hardware Products

Product name | Required options, conditions, etc.
Utility Tray-A2 | Using with Handset-G2 is not available.
Card Reader-F1 | Copy Card Reader Installation Kit-A2 is required. Using with Serial Interface Kit-K1 and Control Interface Kit-A1 is not available.
Copy Card Reader Attachment-B2 | Required when Card Reader-F1 is installed.
Super G3 FAX Board-AK1 | No particular options and conditions are required.
Super G3 2nd Line Fax Board-AK1 | Super G3 FAX Board-AK1 is required.
Super G3 3rd/4th Line Fax Board-AE1 | Super G3 FAX Board-AK1 and Super G3 2nd Line Fax Board-AK1 is required.
Voice Guidance Kit-F2 | Using with Voice Operation Kit-C2 is not available.You cannot use the Voice Guidance Kit when you are logged in using SSO-H authentication.
Voice Operation Kit-C2 | Using with Voice Guidance Kit-F2 is not available.You cannot use the Voice Operation Kit when you are logged in using SSO-H authentication.
USB Device Port-D1 | No particular options and conditions are required.
Additional Memory Type A (512MB) | Required when 600 dpi color scanning (mode) is required.
Heater Kit-K1 | It is needed Heater Kit-K1 when installing the optional heater.
2.5inch/80GB HDD-C1 | This is used when the mirroring function is used with HDD Mirroring Kit-F1 or HDD Data Encryption & Mirroring Kit-C4. No particular options and conditions are required.
2.5inch/250GB HDD-D1 | This is used when the mirroring function is used with HDD Mirroring Kit-F1 or HDD Data Encryption & Mirroring Kit-C4. No particular options and conditions are required.
Removable HDD Kit-AF1 | No particular options and conditions are required.
HDD Mirroring Kit-F1 | Option HDD (2.5 inch/80 GB)-C1 or Option HDD (2.5 inch/250 GB)-D1 are required.
HDD Data Encryption & Mirroring Kit-C4 | When performing mirroring, either the Option HDD (80GB) or the Option HDD (250GB) is required.
Expansion Bus-F2 | Required when /Wireless LAN Board-B1/B2 is installed.
Wireless LAN Board-B2 | No particular options and conditions are required.
Multimedia Reader/Writer-A2 | USB Device Port-D1 is required. To support the CF, the SD memory and the memory stick.
Serial Interface Kit-K1 | Required when the coin manager is connected. Using with Card Reader-F1 and Control Interface Kit-A1 is not available.
Copy Control Interface Kit-A1 | Required when the coin manager is connected. Using with Card Reader-F1 and Serial Interface Kit-K1 is not available.
NE Controller-C1 | No particular options and conditions are required.
eM Controller-C1 | No particular options and conditions are required.
iR-ADV Security Kit-B1 for IEEE 2600.1 Common Criteria Certification | No particular options and conditions are required.
Drum Heater-C1 | Heater Kit-K1 is required.

License Products
At the time of installation, obtain the license number according to the license certificate
included. Then, enter the obtained license number from the Control Panel of the machine, so
that the applicable functions are enabled.
There is no physical installation work at the time of installation.

Product name | Required options, conditions, etc.
PCL Printer Kit-AN1/AN1e | No particular options and conditions are required.
PS Printer Kit-AN1/AN1e | No particular options and conditions are required.
Universal Send Advanced Feature Set-E1/E1e | No particular options and conditions are required.
Universal Send Security Feature Set-D1/D1e | No particular options and conditions are required.
Direct Print Kit (for PDF/XPS)-H1/H1e | No particular options and conditions are required.
Direct Print Kit (for PDF)-H1 | No particular options and conditions are required.
Direct Print Kit (for XPS)-H1 | No particular options and conditions are required.
Universal Send Digital User Signature Kit-C1/C1e | No particular options and conditions are required.
Universal Send Searchable PDF/XPS Kit-D1e | US only No particular options and conditions are required
Universal Send PDF Encryption Kit-D1e | US only No particular options and conditions are required
Remote Operators Software Kit-B1/B1e | No particular options and conditions are required.
Data Erase Kit-C1/C1e | No particular options and conditions are required.
Encrypted Secure Print Software-D1/D1e | No particular options and conditions are required.
Encrypted Printing Software-D1 | No particular options and conditions are required.
Barcode Printing Kit-D1/D1e | No particular options and conditions are required.
Watermark Expansion Kit-B1/B1e | No particular options and conditions are required.
Document Scan Lock Kit-A1 | No particular options and conditions are required.
Access Management System Kit-B1/B1e | No particular options and conditions are required.
Web Access Software-H1/H1e | No particular options and conditions are required.
Remote Fax Kit-A1/A1e | No particular options and conditions are required.
PCL International Font Set-A1/A1e | No particular options and conditions are required.

Universal Send Advanced/Security Feature Set & PS/PCL Print Package-E1

US/CLA/CAN only
The following options are bundled.
PCL Printer Kit-AN1
PS Printer Kit-AN1
Universal Send Advanced Feature Set-E1
Universal Send Security Feature Set-D1