Installation Procedure

| Print out this category

Installation Procedure
1) Remove the Right Rear Cover (Upper).
2 Screws
2 Protrusions
1 Claw
2) Disconnect the USB Cable and the Control Panel Communication Cable.
3) Remove the Main Controller PCB 1.
2 Screws (beside of arrow mark)
1 Connector
CAUTION:
Be sure to move the USB Cable and the Control Panel Communication Cable to the Reader side to prevent the cables from being trapped.
CAUTION:
Be sure to place the removed Main Controller PCB 1 on flat surface.
Reason: Since the fan protrudes, if it is placed at a tilt, it may be damaged.
4) Remove the Screw and the Spacer from the Voice Operation Board Unit. (The removed screw and spacer will not be used.)
5) Remove the Face Plate from the Main Controller PCB 1 (The removed Face Plate will not be used.)
2 Screws (The removed screws will be used in step 6.)
6) Install the Voice Operation Board Unit.
1 Connector
2 Screws (Use the screws removed in step 5)
2 Screws (TP; M3x6)
NOTE:
Check that the connector is connected properly.
7) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
8) Install the USB Cable and Control Panel Communication Cable.
9) Remove the Speaker Unit (Lower) from the Speaker Unit.
2 Screws (The removed screws will be used in step 12.)
10) Remove the Face Seals from the Reader Right Cover. (The removed Face Seals will not be used.)
11) Install the Speaker Unit (Lower).
2 Screws (Binding; M4x14)
12) Install the Speaker Unit (Lower).
2 Screws (Use the screws removed in step 9.)
13) Install the Ring Cores to both ends of the DVI Cable, and remove the cap.
14) Cut off the part of the Right Rear Cover (Upper) shown in the drawing with a flat-blade screwdriver.
15) Connect the DVI Cable to the Speaker Unit.
16) Put the DVI Cable through the Right Rear Cover (Upper), and connect the other end of the DVI Cable.
17) Install the Right Rear Cover (Upper).
2 Screws (Use the screws removed in step 1.)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.
18) Remove the 3 Face Seals, and install the 3 Wire Saddles as shown in the figure.
(The removed Face Seals will not be used.)
19) Secure the DVI Cable using the 3 Wire Saddles as shown in the figure.