Setting for login by RLS Authentication

| Print out this category

Setting for login by RLS Authentication
The procedures for changing the RLS authentication Start/ Stop settings are as follows.
1) In order to make a setting for Login by RLS Authentication, you need to Login by Password Authentication.
URL: https://<IP address of MEAP device>:8443/sms/rls/
Ex.) https://172.16.188.240:8443/sms/rls
Login screen by Password Authentication
2) Select [ System Application Management ] on System Management menu.
3) Click on [ Start ] or [ Stop ] button shown on Status field of SMS Installer Service (Remote Login Service Authentication) to check if the status is changed.
4) Log out and then log in again and access via the RLS authentication login window.
When RLS authentication is set to [ Start ] , another RLS login screen is firstly shown. When accessing to RLS status screen with the setting of [ Stop ] , the user will be redirected to the password authentication screen.
RLS authentication started screen and RLS authentication stopped screen
CAUTION:
In case that the login method to a device is set to SSO-H, if you log in SMS with RLS authentication, no selection is displayed although it is the screen to change the login method.
This is the specification to prevent the inconsistent setting which enables to stop SMS Installer Service (Password Authentication) by changing the login method to Default Authentication.
When you want to change the login method to a device, log in the SMS with the password authentication.