PCBs

| Print out this category

Specifications/configuration
PCBs

Parts name | Function, specifications, features
Main controller PCB 1 | CPU: 1.2 GHz, Control of the entire system Various controls (HDD control, memory, control panel, electric power, voice), I/Fs (PCI, USB(host), USB(devise), LAN), RTC
Flash PCB | Boot program
TPM PCB | To generate and save encryption key Available only when TPM settings is ON: Management Settings> Data Management> TPM Settings (default: OFF) Not available with China models
Main controller PCB 2 | CPU: 400 MHz, Image control Image processing (resolution conversion, image rotation, halftone process, scanner image process, printer image process, compression/decompression, decoding, direct mapping, image area determination, generation of histogram, Trimming, Masking) , USB(devise) control, I/F (Reader, Printer, FAX, HDD, Power supply)
HDD | 2.5 inch SATA I/F Standard: 80 GB Up to 2 HDDs can be mounted in the case of mirroring configuration. BOX data, Address book, security information (password, certificate) Op.: (2.5 inch / 80 GB) HDD-C1, (2.5 inch / 250 GB) HDD-D1