Steps for settings of service call completion

| Print out this category

Steps for settings of service call completion
When the service technician completes the work for the service call, follow the instruction as described below to execute the service call completion work.
1. Start [Service Mode] at Level 1.
For the procedures, see “Steps to E-RDS settings - step 1.“.
2. Select [COPIER] > [Option] > [USER] > [SCALLCMP].
3. Touch the numeric button [1] or [0] on the control panel (the setting value is changed to 1 or 0) and touch the [OK] button. (The data is reflected to the setting value field.)
NOTE:
E-RDS generates an alarm of service call completion at this timing, and sends the alarm to UGW.
NOTE:
In the current condition, touching the [OK] button completes the service call regardless of whether 0 or 1 is set.