DSPLY-SW

| Print out this category

DSPLY-SW

COPIER>OPTION>DSPLY-SW
UI-COPY | Display/hide of copy screen
Lv.2 | Details | To set whether to display or hide the copy function.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
UI-BOX | Display/hide of Inbox screen
Lv.2 | Details | To set whether to display or hide the Inbox function.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: No Inbox function (Storing is not available even with PDL to Inbox.) 1: Inbox function is active 2: Inbox function is active (with limitation; Storing is available with PDL to Inbox despite no display on the Control Panel/remote UI)
Default value | 1
UI-SEND | Display/hide of send screen
Lv.2 | Details | To set whether to display or hide the SEND function.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
UI-FAX | Display/hide of FAX screen
Lv.2 | Details | To set whether to display or hide the FAX function.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
ANIM-SW | [Not used]
UI-PRINT | Display/hide of print job screen
Lv.2 | Details | To set whether to display or hide the print job screen.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
UI-RSCAN | Display/hide of remote scan screen
Lv.2 | Details | To set whether to display or hide the remote scan screen on the Control Panel.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch."
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
UI-EPRNT | Display/hide of extended print screen
Lv.2 | Details | To set whether to display or hide the extended print screen (print screen for print server).
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
UI-WEB | Display/hide of Web browser screen
Lv.2 | Details | To set whether to display or hide the Web browser screen.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
RMT-CNSL | ON/OFF of MEAP console screen
Lv.2 | Details | Selecting "1: ON" enables to obtain log for Function Composer on console screen.
Use case | When obtaining log for Function Composer
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
UI-SBOX | ON/OFF of Advanced Box screen display
Lv.2 | Details | To set ON/OFF of the Advanced Box screen on the Control Panel.
Use case | When not displaying the Advanced Box screen on the Control Panel
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | Europe: 0, Other than Europe: 1
UI-MEM | ON/OFF of memory media screen display
Lv.2 | Details | To set ON/OFF of the memory media screen display on the Control Panel.
Use case | When not displaying the memory media screen on the Control Panel
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
UI-NAVI | Dis/hide of introduce to useful features
Lv.2 | Details | To set whether to display or hide "Introduction to Useful Features" in the main menu.
Use case | Upon user's request
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
UI-MOBP | Display/hide of mobile print
Lv.2 | Details | To set whether to display or hide "Mobile Print" in the main menu.
Use case | Upon user's request
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
UI-CUSTM | ON/OFF of custom menu screen display
Lv.2 | Details | To set ON/OFF of the custom menu screen display on the Control Panel.
Use case | When not displaying the custom menu screen on the Control Panel
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
SDTM-DSP | Display/hide of auto shutdown time
Lv.1 | Details | To set whether to display "Auto Shutdown Time" in user mode.
Use case | Upon user's request
Adj/set/operate method | Enter the setting value, and then press OK key.
Caution | When "Hide" is set, auto shutdown time is reset. (Auto shutdown is not performed.)
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | Europe: 1, Others: 0
Related user mode | Settings/Registration> Preferences> Time/Energy Settings> Auto Shutdown Time