Installation Procedure

| Print out this category

Installation Procedure
1) Remove the Right Rear Cover (Upper).
2 Screws
2 Protrusions
1 Claw
2) Disconnect the USB Cable and the Control Panel Communication Cable.
3) Remove the Main Controller PCB 1.
2 Screws (beside of arrow mark)
1 Connector
CAUTION:
Be sure to move the USB Cable and the Control Panel Communication Cable to the Reader side to prevent the cables from being trapped.
CAUTION:
Be sure to place the removed Main Controller PCB 1 on flat surface.
Reason: Since the fan protrudes, if it is placed at a tilt, it may be damaged.
CAUTION: Point to Note at Installation
Be careful to install the correct Wireless LAN Support Plate.
4) Install the Bulk Head Unit to the Wireless LAN Support Plate.
2 Screws (TP; M3x6) (Included in the Wireless LAN Board)
CAUTION: Point to Note at Installation
Be sure to install the Bulk Head Unit with the flat side of the terminal up.
5) Install the PCI Bus Expansion PCB (Included in the Expansion Bus) in the PCI Expansion Support Plate.
2 Screws (TP; M3x6) (Included in the Expansion Bus Kit)
CAUTION: Note when installing
Be sure to install the PCI Bus Expansion PCB to come under [A] part of PCI Expansion Support Plate.
6) Insert the Wireless LAN Board to the connector of the PCI Bus Expansion PCB, and install it in PCI Expansion Support Plate.
1 Screw (TP; M3x6) (Included in the Wireless LAN Board)
7) Install the 3 PCB Spacers (Included in the Expansion Bus).
8) Remove the Cover Plate from the Main Controller PCB 1 (The removed Cover Plate will not be used).
2 Screws (The removed screws will be used in step 10)
9) Install the PCI Expansion Support Plate assembled in step 6 to the Main Controller PCB 1.
1 Connector
3 Screws (TP; M3x6) (Included in the Expansion Bus Kit)
CAUTION:
When installing the PCI Expansion Support Plate, the Wireless LAN Board may be disconnected from the connector of the PCI Bus Expansion PCB. Check that they are connected properly.
10) Install the Wireless LAN Support Plate assembled in step 4) in the Main Controller PCB 1.
2 Screws (Use the screws removed in step 8)
2 Screws (TP; M3x6) (Included in the Wireless LAN Board)
11) Insert the terminal of Bulk Head Unit into the indicated position.
NOTE:
Make sure that the terminal is securely settled.
12) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
13) Install the USB Cable and Control Panel Communication Cable.
14) Install the Right Rear Cover (Upper). (2 Screws)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.
15) Affix the Antenna Tape to the MFP Antenna and attach it to the Reader.
CAUTION:
Be sure to align the [A] part with the [B] line.
Be sure to attach the antenna to a position where the MFP Antenna will not be caught by the ADF when it is opened and closed.
NOTE: When the Card Reader is installed
Hook the [A] part of the MFP Antenna on the edge [B] of the Copy Card Reader Installation Kit to attach it.
16) Remove the covers of the 3 Cord Guides.
17) Connect the terminal of the MFP Antenna.
18) Remove the release paper, and affix the 3 Cord Guides.
CAUTION:
The position to install the Cord Guide [A], etc. varies when installing in combination with other options. (See NOTE in step 19: "When using in combination with other options".)
19) Put the MFP Antenna Cable through the Cord Guides, and attach the Cord Guide Covers.
CAUTION:
Be sure that the terminal of the MFP Antenna is connected properly.
Be sure to pull the cable slack to the rear side of the host machine.
NOTE: When using in combination with other options

<When using in combination with Copy Card Reader only> Secure the cable in place using the Wire Saddle included in the Card Reader Installation Kit. |
<When using in combination with Voice Guidance> Secure the cable in place using the Cord Guide at the position shown in the figure. (It can be either the one included in the Wireless LAN Board or the one included in the Voice Guidance.) |
<When using in combination with Voice Operation Kit> Secure the cable in place using the Wire Saddle included in the Voice Operation Kit. |

20) Affix the Wireless LAN Indication Label, aligning it with the groove.