CLEANING

| Print out this category

CLEANING

COPIER>FUNCTION>CLEANING
DRM-IDL | Drum cleaning
Lv.2 | Details | To perform the drum cleaning
Use case | When the black spots appear on the copy image in the drum circumference cycle. (Toner adheres on the drum surface.)
Adj/set/operate method | Select the item, and then press OK key.
Required time | 60 seconds
TR-CLN | Transfer roller cleaning
Lv.2 | Details | To clean the transfer roller
Use case | When the back side of paper is soiled with toner (the transfer roller is soiled with toner).
Adj/set/operate method | Select the item, and then press OK key.
Required time | Approx. 35 seconds
FIX-CLN | Fixing film cleaning
Lv.2 | Details | To clean the fixing film
Use case | When the fixing pressure roller is soiled with tonner.
Adj/set/operate method | 1) Print out the cleaning pattern (setting value: 44) with COPIER> TEST> PG> TYPE. 2) Press OK key to execute the cleaning after setting the paper on the manual tray.
Required time | Approx. 60 seconds