Power Configuration of the Heater

| Print out this category

Heater control
Power Configuration of the Heater

Name | Description | Reference value
Heater PCB | The heater PCB is not available as a product for USA/ CAN/ EUR. There is an exclusive built-in cassette heater PCB in the host machine for CSPL/ CHK/ CLA/ CA/ CCN. When installing a heater other than the cassette heater, the cassette heater PCB must be replaced by the heater PCB-K1. |
Reader heater | Reader heater is not available as a product for USA/ CAN/ EUR/ TW. | Surface temperature: About 120-140 deg C Power consumption: About 8.3W (120V) /9.7W(200V)
Drum heater | Drum heater is not available as a product for USA/ CAN/ EUR. | Surface temperature: About 80 deg C Power consumption: About 20W or less
Cassette heater | Cassette heater is not available as a product for USA/ CAN/ EUR. There is a cassette heater in the host machine as a standard feature for CSPL/ CHK/ CLA/ CA/ CCN. | Surface temperature: About 60 deg C Power consumption: About 16W
Deck heater | Deck heater is not available as a product for USA/ CAN/ TW. Deck heater is available as a service part for EUR. | Surface temperature: About 73 deg C Power consumption: About 20W