Overview

| Print out this category

Fan Control
Overview
Fan layout

No. | Name | Function | Error code
FM1 | Fixing film cooling fan (rear) | Cools the fixing unit. Cool paper on the delivery tray | E840-0001 E840-0002
FM2 | Fixing film cooling fan (front) | E840-0003 E840-0004
FM3 | Exhaust fan (rear) | Cools the fixing unit. | E805-0000 E805-0001
FM4 | Exhaust fan (front) | Cools the fixing unit. | E805-0002 E805-0003
FM5 | Power supply cooling fan | Cools the power supply. | E804-0000
FM6 | Main body cooling fan | Cools the power supply. Circulate air in the host machine. | E806-0000 E806-0001
FM7 | Paper cooling fan | Cool paper. | E806-0002 E806-0003
FM12 | Controller cooling fan | Cools the main controller. | E880-0001

*1: The fan operates at half speed only when the machine enters the standby mode after running for more than 8 minutes for fixing.
*2: The fan control in PRINT/LSTR performs full speed/half speed drive/stop depending on print mode and fix control temperature.
<Related service modes>
Change of rotational speed for paper edge cooling fan
(Lv.2) COPIER> ADJUST> FIXING> FN-MV-SW
0: OFF, 1: Half speed (default), 2: Full speed
Fan drive extension mode after job
(Lv.2) COPIER> OPTION> FNC-SW> FAN-EXTN
0:OFF, 1:ON