Work Procedure

| Print out this category

Work Procedure
1) Remove the drum unit, and then attach the drum cover removed during installation.
2) Secure the optical system using the two screws removed during installation.
3) Secure the front cover, toner supply cover, delivery section, and cassette with tape.
4) Place an A3-size sheet on the document glass, and then secure the document glass cover (ADF) with tape.