Installation Procedure

| Print out this category

Installation Procedure
1) Remove the Right Rear Cover (Upper).
2 Screws
2 Protrusions
1 Claw
2) Disconnect the USB Cable and the Control Panel Communication Cable.
3) Remove the Main Controller PCB 1.
2 Screws (beside of arrow mark)
1 Connector
CAUTION:
Be sure to move the USB Cable and the Control Panel Communication Cable to the Reader side to prevent the cables from being trapped.
CAUTION:
Be sure to place the removed Main Controller PCB 1 on flat surface.
Reason: Since the fan protrudes, if it is placed at a tilt, it may be damaged.
4) Remove the Face Plate. (The removed Face Plate will not be used.)
3 Screws (The removed screws will be used in step 6.)
5) Install the PCB Spacer.
6) Install the Card Reader Reply Unit.
3 Screws (Use the screws removed in step 4.)
1 Connector
7) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
8) Install the USB Cable and Control Panel Communication Cable.
9) IInstall the Card Reader Mounting Plate (Rear) to the Card Reader Mounting Plate (Lower).
2 Screws (Binding; M4x6)
10) Remove Short Connector from the connector of the Card Reader Unit. (The removed Short Connector will not be used.)
11) Remove the Lower Cover of the Card Reader Unit, and change the position of the cable by putting it through the groove shown in the figure below.
1 Screws
12) Install the Lower Cover of the Card Reader Unit.
13) Install the Card Reader Unit to the Card Reader Mounting Plate (Front).
2 Bosses
1 Toothed Washer
1 Screw (RS Tightening; M4x10)
1 Wire Saddle
14) Connect the Card Reader External Relay Harness to the connector of the Card Reader Unit.
1 Connector
1 Edge Saddle
CAUTION:
Be sure that the core is inside the Edge Saddle.
15) Install the Card Reader Mounting Plate (Rear) to the Card Reader Mounting Plate (Front).
4 Screws (TP; M3x6)
CAUTION:
Be careful not to trap the harness.
16) Remove the Face Seal from the Reader Right Cover.
17) Install the Card Reader to the host machine.
2 Bosses
2 Screws (Binding; M4x6)
18) Install the Right Rear Cover (Upper). (2 Screws)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.
19) Connect the connector of the Card Reader External Relay Harness to the host machine, and install the Connector Cover.
1 Screw (TP; M3x6)
CAUTION:
When installing the Connector Cover, be sure to place the tie-wrap on the Card Reader External Relay Harness on the inside of the Connector Cover.
20) Remove the Face Seal from the Reader Rear Cover, and install the Wire Saddle. (The removed Face Seal will not be used.)
<When using the Card Reader only>
Use the Wire Saddles included in the package of this equipment.
<When using in combination with the Voice Operation Kit>
Use the 2 Wire Saddles included in the Voice Operation Kit
21) Remove the covers of 2 Cord Guides. (When using in combination with the Voice Operation Kit, use 1 Cord Guide.)
22) Remove the release paper from the Cord Guides, and affix the guides to the 2 areas indicated in the figure.
NOTE:
When using in combination with the Voice Operation Kit, the Cord Guide [A] is not needed.
23) Put the Card Reader External Relay Harness through the Cord Guides, and install the covers of the guides. (When using in combination with the Voice Operation Kit, put the harness through 1 Cord Guide.)
24) Secure the harness in place using the Wire Saddle. (When using in combination with the Voice Operation Kit, secure it with the 2 Wire Saddles.)
25) Connect the power plug of the host machine to the power outlet.
26) Turn ON the main power switch.