Checking the Network Connection

| Print out this category

Checking the Network Connection
CAUTION:
Be sure to use the network cable with Category 5e or higher. In addition, a sealed type (STP cable) is recommended.
Using the non-shield type can affect the peripheral electrical equipment through the network cable.
1) Turn OFF the main power switch.
2) Connect the network cable to the Host Machine and turn ON the main power switch.
3) Inform the system administrator at the installation site that installation of the Host Machine is complete, and then, ask for the network setting.
NOTE:
Network setting cannot be executed unless logging in as an administrator.
Factory default password is as follows.
System administration division ID: 7654321
• System administration password: 7654321
CAUTION:
To perform the network setting, the following Additional Functions items must be set "ON".
[Additional Functions] > [Configuration] > [Network] > [Change network settings/ check connection]
[Additional Functions] > [Configuration] > [Network] > [TCP/IP Setting] > [IPv4 setting] > [Use IPv4]
4) Turn OFF and then ON the main power.