Unpacking the Machine and Removing the Packaging Materials

| Print out this category

Unpacking and Installation Procedure
Unpacking the Machine and Removing the Packaging Materials
1) Unpack the machine and remove the vinyl cover.
NOTE:
When installing the host machine and the options at the same time, install the options first by following the procedure below for better workability.
1. Installing the Cassette Pedestal (Refer to Installation Procedure for the Cassette Pedestal.)
2. Installing the host machine
When installing the host machine and the USB Device Port at the same time, install the USB Device Port before installing the Control Panel (after step 9 of “Installing the Printer Cover”)
2) While holding four handles on the left and right sides of the machine, lift the machine to take it down from the palette.
CAUTION:
The maximum weight of the machine is approx. 58 kg.
Be sure to perform the work in accordance with the standard to handle a heavy
load in each country. In addition, be sure to keep the machine leveled when
lifting it.
3) Remove the tapes on the exterior of the host machine.
CAUTION:
Remove the following in later step.
Cassette inside (wire of the cassette intermediate plate)
Front cover inside (fixing tape of the waste toner container mount)
Right cover inside (fixing pressure release material)
4) Press the cassette release button to draw out the cassette forward.
5) Remove the wire that secures the intermediate plate of the cassette 1/2 and the fixing tape.
6) Insert the cassette 1/2.
7) Press the button on the right cover to open the right cover.
8) Remove the fixing pressure release material.
9) Close the right cover.