When Installing the Serial Interface Kit-K1

| Print out this category

When Installing the Serial Interface Kit-K1
1) Remove the Face Plate. (The removed Face Plate will not be used.)
2 Screws (One of the removed screws will be used in step 4), and the other will not be used.)
2) Install the PCB Spacer.
3) Connect the RS Conversion Cable to the Serial RS Conversion Board.
4) Install the Serial RS Conversion Board.
2 Hexagon Screws
2 Washers
1 Screw (Use one of the screws removed in step 1.)
1 Connector
NOTE:
Be sure to tighten the Hexagon Screw with needlenose pliers.