Fixing film edge cooling control

| Print out this category

Fixing film edge cooling control
When making prints with the paper that the width is shorter than A4, to prevent temperature
rise of non-feeding area, the fan attached near the fixing assembly sends air and cools to
the front and rear side of the fixing film.
For details of the fixing film edge cooling control, see Technology > Controller System >
Controls > Fan.
Related Service Mode
- Setting for down sequence start temperature
COPIER > OPTION > CLEANING
> FX-CN-SW (Set fixing pressure roller cleaning sequence)
> PSP-PR4 (Set productivity priority in rotation collation mode)