ADJUST

| Print out this category

﻿SORTER
ADJUST

SORTER>ADJUST
PNCH-Y | Punch Hole Side-Reg Position Adj: Inner Fin
Lv.1 | Details | To adjust the punch hole position in the side registration direction The punch hole is moved 0.45mm by changing the value. +: towards rear -: towards front
Use case | When the punch hole position is incorrect in the side registration direction
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -50 to 50
Unit | 0.45 mm
Default value | 0
CLCT-SB | Switch Back Amount Adj
Lv.1 | Details | To adjust the switch back amount when the paper is delivered to the process tray
Use case | When the stack failure is caused by the curled paper in the process tray
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -50 to 50
Unit | 0.1 mm
Default value | 0
STP-F1 | Front 1-staple position (R size)
Lv.1 | Details | To adjust the A4R/LGL/LTRR paper front 1-staple position on Finisher. As the value is incremented by 1, the staple position moves by 0.49 mm. +: Toward front -: Toward rear
Use case | When the A4R/LGL/LTRR paper front staple position is displaced
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -6 to 6 (Even if the value out of range is set, the same result as that of maximum/minimum value is expected.)
Unit | 0.49 mm
STP-F2 | Front 1-staple position(half size)
Lv.1 | Details | To adjust the A3/B4/A4/B5/LDR/LTR/EXEC/8K/16K paper front 1-staple position on Finisher. As the value is incremented by 1, the staple position moves by 0.49 mm. +: Toward front -: Toward rear
Use case | When the A3/B4/A4/B5/LDR/LTR/EXEC/8K/16K paper front staple position is displaced
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -6 to 6 (Even if the value out of range is set, the same result as that of maximum/minimum value is expected.)
Unit | 0.49 mm
STP-R1 | Rear 1-staple position (R size)
Lv.1 | Details | To adjust the A4R/LGL/LTRR paper rear 1-staple position on Finisher. As the value is incremented by 1, the staple position moves by 0.49 mm. +: Toward front -: Toward rear
Use case | When the A4R/LGL/LTRR paper rear staple position is displaced
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -6 to 6 (Even if the value out of range is set, the same result as that of maximum/minimum value is expected.)
Unit | 0.49 mm
STP-R2 | Rear 1-staple position (half size)
Lv.1 | Details | To adjust the A3/B4/A4/B5/LDR/LTR/EXEC/8K/16K paper rear 1-staple position on Finisher. As the value is incremented by 1, the staple position moves by 0.49 mm. +: Toward front -: Toward rear
Use case | When the A3/B4/A4/B5/LDR/LTR/EXEC/8K/16K paper rear staple position is displaced
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -6 to 6
Unit | 0.49 mm
STP-2P | Adj front/rear 2-staple position
Lv.1 | Details | To adjust the front/rear 2-staple position on Finisher. As the value is incremented by 1, the staple position moves by 0.1mm. +: Toward front -: Toward rear
Use case | When the front/rear 2-staple position is displaced
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -50 to 50
Unit | 0.1 mm
PNCH-X | Punch hole position in feed way
Lv.1 | Details | To adjust the punch hole position on Finisher in feed direction. As the value is incremented by 1, the punch hole moves by 0.1mm. +: Toward delivery direction -: Toward inlet direction
Use case | When the punch hole is displaced in feed direction
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -50 to 50
Unit | 0.1 mm
Appropriate target value | 0
SDL-STP | Adj of Saddle Stitcher staple position
Lv.1 | Details | To adjust the staple position of Saddle Stitcher. As the value is incremented by 1, the staple position moves by mm.
Use case | When the staple position of the Saddle Stitcher is displaced
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -3 to 3
Unit | mm
Default value | 0
SDL-ALG | Adj of Saddle Stitcher alignment width
Lv.1 | Details | To adjust the alignment width of Saddle Stitcher. As the value is incremented by 1, the alignment width is increased by mm.
Use case | When the misalignment occurs within a paper stack on the Saddle Stitcher
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1
Unit | mm
Default value | 0
ST-ALG1 | Adj Stacker A4 size align pstn:Finisher
Lv.1 | Details | To adjust the A4 size paper alignment position. As the value is incremented by 1, the travel length of the Alignment Plate is increased by 0.42mm.
Use case | When misalignment occurs in A4 size paper
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -10 to 10
Unit | 0.42 mm
Appropriate target value | 0
Default value | 0
SW-UP-RL | Adj Swing Roller falling pstn: Finisher
Lv.1 | Details | To adjust the Swing Roller fall position. As the value is incremented by 1, the Swing Roller fall position moves downward by 0.2mm.
Use case | When paper fails to be transported to the Processing Tray and misalignment occurs
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -17 to 33
Unit | 0.2 mm
Appropriate target value | 0
Default value | 0
PUN-V-RG | Adj punch vertical rgst pstn: External Puncher
Lv.1 | Details | To adjust the vertical registration position of the paper to be punched. As the value is incremented by 1, the punch hole position moves toward the edge by 1mm.
Use case | When misalignment of punch hole position occurs
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -4 to 2
Unit | 1 mm
Appropriate target value | 0
Default value | 0
PRCS-RET | Adj Process Tray return amount:Finisher
Lv.1 | Details | To adjust the pull-back amount of the paper on the Processing Tray. As the value is incremented by 1, the pull-back amount is decreased by 1.4mm.
Use case | When the paper is bent in the Processing Tray
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 5
Unit | 1.4 mm
Appropriate target value | 0
Default value | 0
UP-CL | Upward curl prevention mode: Finisher
Lv.1 | Details | Set 1 when upward curl occurs on the paper delivered to the Stack Tray, and paper leaning due to the curl occurs.
Use case | When upward curl occurs on the paper delivered to the Stack Tray, and paper leaning due to the curl occurs
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
DW-CL | Downward curl prevention mode: Finisher
Lv.1 | Details | Set 1 when downward curl occurs on the paper delivered to the Stack Tray, and paper leaning due to the curl occurs.
Use case | When downward curl occurs on the paper delivered to the Stack Tray, and paper leaning due to the curl occurs
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
THC-CL | Heavy ppr curl prevention mode:Finisher
Lv.1 | Details | Set 1 when upward curl occurs on the heavy paper delivered. When 1 is set, the amount of Stack Tray dissension for stack delivery increases. The paper surface detection is performed for every sheet, not for every 5 sheets.
Use case | When upward curl occurs on the heavy paper delivered
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
THC-PUSH | Heavy ppr out prevention mode:Finisher
Lv.1 | Details | Set 1 when the already stacked paper is pushed out at the time of heavy paper delivery. When 1 is set, the Stack Tray moves down temporarily before the heavy paper is delivered to the Processing Tray if the leading sheet is heavy paper.
Use case | When the already stacked paper is pushed out at the time of heavy paper delivery
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
OFST-STC | Poor offset stack prev mode:Finisher
Lv.1 | Details | Set 1 when paper is not appropriately stacked in the small-size offset mode. When 1 is set, buffer operation is not performed in the small-size offset mode.
Use case | When paper is not appropriately stacked in the small-size offset mode
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
THN-STC | Poor thin ppr stack prev mode:Finisher
Lv.1 | Details | Set 1 when thin paper is not appropriately stacked. When 1 is set, the stacking condition of thin paper improves.
Use case | When thin paper is not appropriately stacked
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
STP-P-CH | Stpl stack displace prev mode:Finisher
Lv.1 | Details | Set 1 when the paper on the top is misaligned in the staple delivery mode. When 1 is set, paper stack alignment operation is executed twice immediately before stapling.
Use case | When the paper on the top is misaligned in the staple delivery mode
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
TRY-NIS | Tray switch noise reduct mode:Finisher
Lv.1 | Details | Set 1 when the operation noise after switching the Stack Tray is loud. When 1 is set, the Stack Tray rise operation becomes slow.
Use case | When the operation noise after switching the Stack Tray is loud
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
TRY-SU | Tray switching speedup mode: Finisher
Lv.1 | Details | Set 1 when the Stack Tray switching time is long. When 1 is set, the Stack Tray rise speed becomes fast.
Use case | When the Stack Tray switching time is long
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
FIN-NIS | Tray drive noise reduct mode: Finisher
Lv.1 | Details | Set 1 when the Finisher operation noise is loud. When 1 is set, the initial Finisher operation is minimized.
Use case | When the Finisher operation noise is loud
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
1SHT-SHF | Set 1-sheet Offset+Collate: Finisher
Lv.1 | Details | Set 1 when setting Offset and Collate for 1-sheet document.
Use case | When setting Offset and Collate for 1-sheet document
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
SDL-SWCH | Sddl stck capacity switch mode:Finisher
Lv.1 | Details | Set 1 when increasing the stacking capacity for saddle stitching. When 1 is set, the stacking capacity increases over the upper limit.
Use case | When increasing the stacking capacity for saddle stitching
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
SDL-ALM | Saddle full stack alarm mode: Finisher
Lv.1 | Details | Set 1 when disabling the stack full alarm for saddle stitching.
Use case | When disabling the stack full alarm for saddle stitching
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: ON, 1: OFF
Default value | 0
SFT-AMT1 | Adj shft amnt of Shft Roll (frt)
Lv.1 | Details | To adjust the front shift amount of the Shift Roller. As the value is incremented by 1, the Shift Roller moves toward the guide by 0.1 mm.
Use case | When the front shift amount of the paper is inappropriate
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -50 to 50
Unit | 0.1mm
Default value | 0
SFT-AMT2 | Adj shft amnt of Shft Roll (Rear)
Lv.1 | Details | To adjust the rear shift amount of the Shift Roller. As the value is incremented by 1, the Shift Roller moves toward the guide by 0.1 mm. (The paper length to be detected is shortened by 0.1mm.)
Use case | When the rear shift amount of the paper is inappropriate
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -50 to 50
Unit | 0.1mm
Default value | 0
STP-NTN | Adj of Staple Needle pitch (A4)
Lv.1 | Details | To adjust the pitch between needles for 2-point stapling. As the value is incremented by 1, the pitch between needles becomes wider by 0.27 mm.
Use case | When the pitch between needles for 2-point stapling is inappropriate
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -8 to 8
Unit | 0.27 mm
Default value | 0
INSTP-F1 | Adj of front staple position
Lv.1 | Details | To adjust the paper pull-in amount of the Gripper at the time of front 1-point stapling. As the value is incremented by 1, the paper pull-in amount is increased by 0.1 mm.
Use case | When misalignment occurs at the front staple position
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -50 to 50
Unit | 0.1 mm
Default value | 0
INSTP-R1 | Adj of rear staple position
Lv.1 | Details | To adjust the paper pull-in amount of the Gripper at the time of rear 1-point stapling. As the value is incremented by 1, the paper pull-in amount is increased by 0.1 mm.
Use case | When misalignment occurs at the rear staple position
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | -50 to 50
Unit | 0.1 mm
Default value | 0
THN-STCL | Poor large/thin ppr stack prev mode:Finisher
Lv.1 | Details | Set 1 when large/thin paper is not appropriately stacked. When 1 is set, the stacking condition of large/thin paper improves.
Use case | When large/thin paper is not appropriately stacked
Adj/set/operate method | Enter the setting value, and then press OK key.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1