CUSTOM

| Print out this category

CUSTOM

COPIER>OPTION>CUSTOM
CCD-TYPE | Setting of CCD Unit type
Lv.2 | Details | To set the CCD Unit type installed in the Reader to the backup area in the controller. Controller switches the image processing table according to the setting value.
Use case | When changing the CCD Unit type
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Initial type, 1: Improved type
Default value | 0
Supplement/memo | If the CCD Unit is changed after factory shipment, the Reader cannot identify the type.
FACT-DEF | Set batch chng of factory setting values
Lv.2 | Details | To set the batch change of factory setting values for customization.
Display/adj/set range | 0 to 1
Default value | 0
MAILYEAR | Set auto add to e-mail Subject/File name
Lv.2 | Details | To set whether to add date, time and split number automatically to the end of a character string of e-mail Subject/File name.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Following the current setting, 1: Adding
Default value | 0
BOX-BKUP | Set to allow Inbox backup data restore
Lv.1 | Details | To set whether to permit restoration of Inbox backup data. Machine subject to restoration can be selected from either the same model or the next model. When restoration is completed normally, the setting value is returned to 0.
Use case | At replacement, permit to restore backup data of other model (some models).
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Permit restoration only from own device to own device (same model only) 1: Permit restoration only from old device to new device (next model only)
Default value | 0
ABK-TOOL | Allow access from address book mntc tool
Lv.1 | Details | To set whether to accept import from the address book maintenance tool.
Use case | When executing import from the address book maintenance tool
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
Supplement/memo | Address book maintenance tool: Tool provided from CMJ.
FLK-RD | Flicker reduction mode
Lv.2 | Details | To change the fixing temperature control to cancel fluorescent flicking during printing
Use case | When the fluorescent flicking occurs during printing
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0
TMP-TBL | Shortening FCOT
Lv.2 | Details | To lower the fixing temperature for the paper feed start during the first copying (-40degC)
Use case | To shorten the first copy time, the fixing temperature for the paper feed start is lowered ( -40degC).
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0