CCD

| Print out this category

CCD

COPIER>ADJUST>CCD
W-PLT-X | White level data(X) entry of white plate
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label. When replacing the Copyboard Glass, enter the value of barcode label which is affixed on the glass.
Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data - When replacing the Copyboard Glass
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Do not use this at the normal service.
Display/adj/set range | 1 to 9999
Default value | 8271
Related service mode | COPIER.> ADJUST> CCD> W-PLT-Y, W-PLT-Z
W-PLT-Y | White level data(Y) entry of white plate
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label. When replacing the Copyboard Glass, enter the value of barcode label which is affixed on the glass.
Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data - When replacing the Copyboard Glass
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 1 to 9999
Default value | 8735
Related service mode | COPIER.> ADJUST> CCD> W-PLT-X, W-PLT-Z
W-PLT-Z | White level data(Z) entry of white plate
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label. When replacing the Copyboard Glass, enter the value of barcode label which is affixed on the glass.
Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data - When replacing the Copyboard Glass
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 1 to 9999
Default value | 9418
Related service mode | COPIER.> ADJUST> CCD> W-PLT-X, W-PLT-Y
SH-TRGT | Shading target value (B&W) [Copyboard]
Lv.1 | Details | To set the B&W shading target value in copyboard reading mode.
Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data - When replacing the Scanner Unit
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 1 to 2047
Default value | 1126
50-RG | clr displace offset value display(R-G)
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
50-GB | clr displace offset value display(G-B)
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
100-RG | Img Sensr RG color displace crrct:Rear
Lv.1 | Details | To correct the color displacement (R and G lines) in vertical scanning direction due to the Scanner Unit. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
100-GB | Img Sensr GB color displace crrct:Rear
Lv.1 | Details | To correct the color displacement (G and B lines) in vertical scanning direction due to the Scanner Unit. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Default value | 0
50DF-GB | Color displacement (G-B) offset VL display at ADF mod/50% scanning
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Default value | 0
100DF-RG | Color displacement (G-R) offset VL display at ADF mod/100% scanning
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Default value | 0
100DF-GB | Color displacement (G-B) offset VL display at ADF mod/100% scanning
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Default value | 0
DFTAR-R | Shading target value (R)
Lv.1 | Details | When replacing the Reader Controller PCB, enter the value of service label. When replacing the Copyboard Glass/Scanner Unit (paper front), execute COPIER> FUNCTION> CCD> DF-WLVL3, DF-WLVL4 and write the value which is automatically set in the service label.
Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data - When replacing the Copyboard Glass/Scanner Unit (paper front)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 2047
Default value | 1159
Related service mode | COPIER> FUNCTION> CCD> DF-WLVL3, DF-WLVL4
Details | When replacing the Reader Controller PCB, enter the value of service label. When replacing the Copyboard Glass/Scanner Unit (paper front), execute COPIER> FUNCTION> CCD> DF-WLVL3, DF-WLVL4 and write the value which is automatically set in the service label.
Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data - When replacing the Copyboard Glass/Scanner Unit (paper front)
Adj/set/operate method | "1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch."
Display/adj/set range | 1 to 2047
Default value | 1189
Related service mode | COPIER> FUNCTION> CCD> DF-WLVL3, DF-WLVL4
DFTAR-B | Shading target value (B)
Lv.1 | Details | When replacing the Reader Controller PCB, enter the value of service label. When replacing the Copyboard Glass/Scanner Unit (paper front), execute COPIER> FUNCTION> CCD> DF-WLVL3, DF-WLVL4 and write the value which is automatically set in the service label.
Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data - When replacing the Copyboard Glass/Scanner Unit (paper front)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 2047
Default value | 1209
Related service mode | COPIER> FUNCTION> CCD> DF-WLVL3, DF-WLVL4
CCD-CHNG | Scanner Unit(ppr frt) rplce flag setting
Lv.1 | Details | To set the calculation mode of MTF filter coefficient that is used at the replacement of Scanner Unit. When replacing the Scanner Unit (paper front), enter 1. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | - When replacing the Scanner Unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Data at factory shipment is used. 1: Data at factory shipment is not used. (Scanner Unit is already replaced.)
Default value | 0
DFTAR-K | Shading target value (Black) at ADF mode
Lv.1 | Use case | - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 2047
Default value | 55
Related service mode | COPIER > FUNCTION > CCD > DF-WLVL1 COPIER > FUNCTION > CCD > DF-WLVL2
MTF3-M1 | MTF setting value for R in horizontal scanning direction (front)
Lv.1 | Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M2 | MTF setting value for R in horizontal scanning direction (center)
Lv.1 | Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M3 | MTF setting value for R in horizontal scanning direction (rear)
Lv.1 | Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M4 | MTF setting value for G in horizontal scanning direction (front)
Lv.1 | Details | Setting value for MTF filter coefficient calculation. Enter the value of service label on the Reader.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M5 | MTF value 5 setting: horz scan [Front]
Lv.1 | Details | MTF setting value for G in horizontal scanning direction (center)
Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M6 | MTF setting value for G in horizontal scanning direction (rear)
Lv.1 | Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M7 | MTF setting value for B in horizontal scanning direction (front)
Lv.1 | Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M8 | MTF setting value for B in horizontal scanning direction (center)
Lv.1 | Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M9 | MTF setting value for B in horizontal scanning direction (rear)
Lv.1 | Use case | Enter the value of service label on the CCD unit in the following cases. - When replacing the CCD unit - When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M10 | MTF setting value for K in horizontal scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M11 | MTF setting value for K in horizontal scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-M12 | MTF setting value for K in horizontal scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S1 | MTF setting value for R in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S2 | MTF setting value for R in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S3 | MTF setting value for R in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S4 | MTF setting value for G in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S5 | MTF setting value for G in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S6 | MTF setting value for G in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S7 | MTF setting value for B in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S8 | MTF setting value for B in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S9 | MTF setting value for B in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch."
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S10 | MTF setting value for K in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S11 | MTF setting value for K in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF3-S12 | MTF setting value for K in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M1 | MTF setting value for R in horizontal scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M2 | MTF setting value for R in horizontal scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M3 | MTF setting value for R in horizontal scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M4 | MTF setting value for G in horizontal scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M5 | MTF value 5 setting: horz scan [Front]
Lv.1 | Details | MTF setting value for G in horizontal scanning direction (center)
Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M6 | MTF setting value for G in horizontal scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M7 | MTF setting value for B in horizontal scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M8 | MTF setting value for B in horizontal scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M9 | MTF setting value for B in horizontal scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M10 | MTF setting value for K in horizontal scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M11 | MTF setting value for K in horizontal scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-M12 | MTF setting value for K in horizontal scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S1 | MTF setting value for R in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S2 | MTF setting value for R in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S3 | MTF setting value for R in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S | MTF setting value for G in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S5 | MTF setting value for G in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S6 | MTF setting value for G in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S7 |  | MTF setting value for B in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S8 | MTF setting value for B in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S9 | MTF setting value for B in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S10 | MTF setting value for K in vertical scanning direction (front)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S11 | MTF setting value for K in vertical scanning direction (center)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
MTF4-S12 | MTF setting value for K in vertical scanning direction (rear)
Lv.1 | Use case | not used usually
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | 20 to 80
Default value | 55
100-GB-2 | Img Sensr G-B color displace crrct (center)
Lv.1 | Details | To correct the color displacement (G and B lines) in vertical scanning direction due to the Scanner Unit. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service labe
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
100-GB-3 | Img Sensr G-B color displace crrct (front)
Lv.1 | Details | To correct the color displacement (G and B lines) in vertical scanning direction due to the Scanner Unit. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
100-RG-2 | Img Sensr R-G color displace crrct (center)
Lv.1 | Details | To correct the color displacement (G and B lines) in vertical scanning direction due to the Scanner Unit. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
100-RG-3 | Img Sensr R-G color displace crrct (front)
Lv.1 | Details | To correct the color displacement (G and B lines) in vertical scanning direction due to the Scanner Unit. When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
50-GB-2 | clr displace offset value display(G-B)
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
50-GB-3 | clr displace offset value display(G-B)
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
50-RG-2 | clr displace offset value display(R-G)
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0
50-RG-3 | clr displace offset value display(R-G)
Lv.1 | Details | When replacing the CCD unit (CCD PCB)/clearing RAM data, enter the value of service label.
Use case | When replacing the CCD unit (CCD PCB)/clearing RAM data
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -256 to 256
Unit | 0.001 line
Default value | 0