﻿Laser Scanner Unit

| Print out this category

Laser Scanner Unit
<Procedure>
"Removing the Laser Scanner Unit."
<Processing after replacing the parts>
When replacing the laser unit, enter the values recorded on the label affixed to the laser unit to be replaced for the following in the service mode:
Adjust of write start position of laser
A.(LV1) COPIER > ADJUST > LASER > PVE-OFST > 136
Difference in magnification between the lasers.
B.(LV1) COPIER > ADJUST > LASER > LDADJ1-K > -10
C.(LV1) COPIER > ADJUST > LASER > LDADJ2-K > 0
D.(LV1) COPIER > ADJUST > LASER > LDADJ3-K > 147
Difference in the phase between the lasers
E.(LV1) COPIER > ADJUST > LASER > LDADJ4-K > 93
F.(LV1) COPIER > ADJUST > LASER > LDADJ5-K > 16
G.(LV1) COPIER > ADJUST > LASER > LDADJ6-K > 117