Product Specifications

| Print out this category

Specifications
Product Specifications

Item | Specifications
Copyboard | Stream reading, original fixed reading
Body | Desktop
Light source type | LED (white)
Photosensitive medium | OPC drum (30 mm dia)
Image reading method | CCD
Reproduction method | Indirect electrostatic method
Exposure method | Laser exposure system
Charging method | Roller charge
Development method | Dry single component projection developing
Transfer method | By transfer roller
Separation method | Curvature and static eliminator
Pickup method | Cassette: Retard separation method Manual feed pickup tray: Pad separation method
Fixing method | On demand
Delivery method | Face down delivery (in-body delivery)
Reproduction ratio | 25% to 400%
Drum cleaning method | By cleaning blade
Toner type | Magnetic negative charge toner
Toner replenish method | Toner cartridge
Toner level detection function | Yes
Image margin | Top margin: 4.0 +1.5mm/-1.0mm Left margin: 2.5±1.5mm
Non-Image Width | Leading Edge Non-Image Width: 4.0 +1.5mm/-1.0mm Left Non-Image Width: 2.5±1.5mm (2.5±2.0mm in ADF mode)
Warm-up time | 38 sec. or less (*1) When the room temperature is 20 degree C *1: Until the copy button is displayed on the top menu from when the operation display becomes effective after turning the power supply ON.
Number of gradations | 256 gradations
Reading resolution | 600×600dpi
Writing resolution | 1200×1200dpi
First print time | iR ADVANCE 4051: 3.7 sec or less iR ADVANCE 4045/4035: 3.8 sec or less iR ADVANCE 4025: 5.2 sec or less
Paper type (Cassette) | plain paper 1 (60 g/m2 to 63 g/m2), plain paper 2 (64 g/m2 to 90 g/m2), recycled paper, color paper, pre-punched paper, heavy paper 1 (91 g/m2 to 105 g/m2), heavy paper 2 (106 g/m2 to 128 g/m2)
Paper type (Manual feed pickup tray) | transparency (52 g/m2 to 59 g/m2),plain paper 1 (60 g/m2 to 63 g/m2), plain paper 2 (64 g/m2 to 90 g/m2), recycled paper, color paper, pre-punched paper, heavy paper 1 (91 g/m2 to 105 g/m2), heavy paper 2 (106 g/m2 to 128 g/m2), heavy paper 3 (129 g/m2 to 163 g/m2), heavy paper 4 (164 g/m2 to 220 g/m2), bond paper, labels, OHP, Envelopes (No.10 (COM10), ISO-B5, Monarch, ISO-C5, DL)
Paper size (Cassette 1) | A4, A4R, A5R, B4, B5, B5R, LTR, LTTR, LGL, STMTR, 8K, 16K, 16KR, EXEC
Paper size (Cassette 2) | Standard size (A3, B4, A4, A4R, B5, B5R, A5R, 8K, 16K,16KR, 279mmX432mm(11"X17"), LGL, LTR, LTRR, STMTR, EXEC, 304mmX457mm(12"X18")) Envelopes* (No.10 (COM10), ISO-B5, Monarch, ISO-C5, DL) * The optional Envelope Feeder Attachment-D1 is required.
Paper size (Manual feed pickup tray) | Cassette feedable size Custom paper size (99 mm x 148 mm to 297 mm x 431 mm)
Pickup capacity | Cassette: 550 sheets (80g/m2), 680 sheets (64g/m2) Manual feed pickup tray: 80 sheets (80g/m2)
Duplex method | Through path duplex
Memory capacity | For Main Controller 1: 1GB (standard)
For Main Controller 2: Max. 1GB (standard: 256MB, option: 768MB)
HDD capacity | Standard: 80GB, Maximum: 250 GB
Environment temperature range | Refer to "Installation" in Chapter
Environment humidity range
Environment atmosphere range | 610 to 1013 hpa (0.6 to 1.0 atmospheric pressure)
Noise (At the time of printing) | iR ADVANCE 4051: 76.85 dB or less iR ADVANCE 4045: 74.75 dB or less iR ADVANCE 4035: 71.25 dB or less iR ADVANCE 4025: 67.75 dB or less
Rated power supply | iR ADVANCE 4051: AC120V/10.4A, AC230V/5.6A iR ADVANCE 4045/35: AC120V/9.3A, AC230V/5.2A iR ADVANCE 4025: AC120V/7.0A, AC230V/4.3A *All the optional power supplies are supplied by the main body.

Power consumption

Maximum power consumption

120-127V:
iR ADVANCE 4051/4045/4035: 1.5kW or less
iR ADVANCE 4025: 1.3kW or less
220-240V:
iR ADVANCE 4051/4045/4035: 1.5kW or less
iR ADVANCE 4025: 1.2kW or less

At the time of printing

120-127V:
iR ADVANCE 4051/4045/4035: 1050.0Wh (Reference)
iR ADVANCE 4025: 688.4Wh (Reference)
220-240V:
iR ADVANCE 4051/4045/4035: 944.0Wh (Reference)
iR ADVANCE 4025: 681.8Wh (Reference)

At the time of sleep (Deep Sleep) | 1.0 W or less (In environmental heater switch OFF)

At the time of standby

120-127V:
iR ADVANCE 4051/4045/4035: 80.9Wh (Reference)
iR ADVANCE 4025: 78.2Wh (Reference)
220-240V:
iR ADVANCE 4051/4045/4035: 101.9Wh (Reference)
iR ADVANCE 4025: 103.2Wh (Reference)

Dimension (WxDxH) | 565mm × 708mm × 769mm (with the platen cover) 565mm × 708mm × 902mm (with the DADF)
Weight | Max (with the DADF): Approx. 77.9 kg Min (without the reader for EU): Approx 58 kg