Buffer Pass Unit-H1

| Print out this category

Buffer Pass Unit-H1

ACC ID | Jam Code | Type | Sensor ID | Sensor Name/Description
00 | 0111 | DELAY | PS1 | Paper in sensor
00 | 0112 | DELAY | PS2 | Paper out sensor
00 | 0211 | STNRY | PS1 | Paper in sensor
00 | 0212 | STNRY | PS2 | Paper out sensor
00 | 0A11 | POWER ON | PS1 | Paper in sensor
00 | 0A12 | POWER ON | PS2 | Paper out sensor
00 | FF11 | SEQ NG*1 | PS1 | Paper in sensor
00 | FF12 | SEQ NG*1 | PS2 | Paper out sensor

*1: The state is recovered by opening and closing the Door, or turning OFF and then ON the power supply.
If it is not recovered by the above operation, it is considered an error near the target sensor.
Disconnect and then connect the connectors around the target sensor, check if the cable is open circuit, and replace the sensor.