Affixing the Labels to the Reader

| Print out this category

Affixing the Labels to the Reader
1) If the following labels are supplied, go through the steps described below.
• Glass cleaning/lamp caution label
• Copy inhibition label
2) Open the pressure plate/DADF.
3) Affix the copy inhibition label [A] (written in an appropriate language) to the existing label.
4) Affix the glass cleaning/lamp caution label [B] written in an appropriate language.