CST

| Print out this category

CST

COPIER>FUNCTION>CST
MF-A4R | Reg Multi-purpose Tray A4R standard width
Lv.1 | Details | To register the standard value of A4R paper width (210mm) on the Multi-purpose Tray. Make a fine adjustment by COPIER> ADJUST> CST-ADJ> MF-A4R.
Adj/set/operate method | 1) Set A4R paper on the Multi-purpose Tray, and set the guide so that it fits the paper width. 2) Select the item, and then press OK key. The value is registered after automatic adjustment.
Caution | After execution, check the registered value by COPIER> ADJUST> CST-ADJ> MF-A4R, and write it down on the service label.
Related service mode | COPIER> ADJUST> CST-ADJ> MF-A4R
MF-A6R | Reg Multi-purpose Tray A6R stdrd width
Lv.1 | Details | To register the standard value of A6R paper width (105 mm) on the Multi-purpose Tray. Make a fine adjustment by COPIER> ADJUST> CST-ADJ> MF-A6R.
Adj/set/operate method | 1) Set A6R paper on the Multi-purpose Tray, and set the guide so that it fits the paper width. 2) Select the item, and then press OK key. The value is registered after automatic adjustment.
Caution | After execution, check the registered value by COPIER> ADJUST> CST-ADJ> MF-A6R, and write it down on the service label.
Related service mode | COPIER> ADJUST> CST-ADJ> MF-A6R
MF-A4 | Reg Multi-purpose Tray A4 standard width
Lv.1 | Details | To register the standard value of A4 paper width (297 mm) on the Multi-purpose Tray. Make a fine adjustment by COPIER> ADJUST> CST-ADJ> MF-A4.
Adj/set/operate method | 1) Set A4 paper on the Multi-purpose Tray, and set the guide so that it fits the paper width. 2) Select the item, and then press OK key. The value is registered after automatic adjustment.
Caution | After execution, check the registered value by COPIER> ADJUST> CST-ADJ> MF-A4, and write it down on the service label.
Related service mode | COPIER> ADJUST> CST-ADJ> MF-A4